--- a/arch/mips/ath79/mach-ubnt-xm.c
+++ b/arch/mips/ath79/mach-ubnt-xm.c
@@ -12,16 +12,24 @@
 
 #include <linux/init.h>
 #include <linux/pci.h>
+#include <linux/platform_device.h>
 #include <linux/ath9k_platform.h>
+#include <linux/etherdevice.h>
+#include <linux/ar8216_platform.h>
 
+#include <asm/mach-ath79/ath79.h>
 #include <asm/mach-ath79/irq.h>
+#include <asm/mach-ath79/ar71xx_regs.h>
 
+#include "common.h"
 #include "dev-ap9x-pci.h"
+#include "dev-eth.h"
 #include "dev-gpio-buttons.h"
 #include "dev-leds-gpio.h"
 #include "dev-m25p80.h"
+#include "dev-usb.h"
+#include "dev-wmac.h"
 #include "machtypes.h"
-#include "pci.h"
 
 #define UBNT_XM_GPIO_LED_L1		0
 #define UBNT_XM_GPIO_LED_L2		1
@@ -37,19 +45,19 @@
 
 static struct gpio_led ubnt_xm_leds_gpio[] __initdata = {
 	{
-		.name		= "ubnt-xm:red:link1",
+		.name		= "ubnt:red:link1",
 		.gpio		= UBNT_XM_GPIO_LED_L1,
 		.active_low	= 0,
 	}, {
-		.name		= "ubnt-xm:orange:link2",
+		.name		= "ubnt:orange:link2",
 		.gpio		= UBNT_XM_GPIO_LED_L2,
 		.active_low	= 0,
 	}, {
-		.name		= "ubnt-xm:green:link3",
+		.name		= "ubnt:green:link3",
 		.gpio		= UBNT_XM_GPIO_LED_L3,
 		.active_low	= 0,
 	}, {
-		.name		= "ubnt-xm:green:link4",
+		.name		= "ubnt:green:link4",
 		.gpio		= UBNT_XM_GPIO_LED_L4,
 		.active_low	= 0,
 	},
@@ -66,9 +74,13 @@ static struct gpio_keys_button ubnt_xm_g
 	}
 };
 
+#define UBNT_M_WAN_PHYMASK	BIT(4)
+
 static void __init ubnt_xm_init(void)
 {
 	u8 *eeprom = (u8 *) KSEG1ADDR(UBNT_XM_EEPROM_ADDR);
+	u8 *mac1 = (u8 *) KSEG1ADDR(0x1fff0000);
+	u8 *mac2 = (u8 *) KSEG1ADDR(0x1fff0000 + ETH_ALEN);
 
 	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_xm_leds_gpio),
 				 ubnt_xm_leds_gpio);
@@ -79,9 +91,428 @@ static void __init ubnt_xm_init(void)
 
 	ath79_register_m25p80(NULL);
 	ap91_pci_init(eeprom, NULL);
+
+	ath79_register_mdio(0, ~UBNT_M_WAN_PHYMASK);
+	ath79_init_mac(ath79_eth0_data.mac_addr, mac1, 0);
+	ath79_init_mac(ath79_eth1_data.mac_addr, mac2, 0);
+	ath79_register_eth(0);
 }
 
 MIPS_MACHINE(ATH79_MACH_UBNT_XM,
 	     "UBNT-XM",
 	     "Ubiquiti Networks XM (rev 1.0) board",
 	     ubnt_xm_init);
+
+MIPS_MACHINE(ATH79_MACH_UBNT_BULLET_M, "UBNT-BM", "Ubiquiti Bullet M",
+	     ubnt_xm_init);
+
+static void __init ubnt_rocket_m_setup(void)
+{
+	ubnt_xm_init();
+	ath79_register_usb();
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_ROCKET_M, "UBNT-RM", "Ubiquiti Rocket M",
+	     ubnt_rocket_m_setup);
+
+static void __init ubnt_nano_m_setup(void)
+{
+	ubnt_xm_init();
+	ath79_register_eth(1);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_NANO_M, "UBNT-NM", "Ubiquiti Nanostation M",
+	     ubnt_nano_m_setup);
+
+static struct gpio_led ubnt_airrouter_leds_gpio[] __initdata = {
+	{
+		.name		= "ubnt:green:globe",
+		.gpio		= 0,
+		.active_low	= 1,
+	}, {
+	        .name		= "ubnt:green:power",
+		.gpio		= 11,
+		.active_low	= 1,
+		.default_state  = LEDS_GPIO_DEFSTATE_ON,
+	}
+};
+
+static void __init ubnt_airrouter_setup(void)
+{
+	u8 *mac1 = (u8 *) KSEG1ADDR(0x1fff0000);
+	u8 *ee = (u8 *) KSEG1ADDR(0x1fff1000);
+
+	ath79_register_m25p80(NULL);
+	ath79_register_mdio(0, ~UBNT_M_WAN_PHYMASK);
+
+	ath79_init_mac(ath79_eth0_data.mac_addr, mac1, 0);
+	ath79_init_local_mac(ath79_eth1_data.mac_addr, mac1);
+
+	ath79_register_eth(1);
+	ath79_register_eth(0);
+	ath79_register_usb();
+
+	ap91_pci_init(ee, NULL);
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_airrouter_leds_gpio),
+				 ubnt_airrouter_leds_gpio);
+
+	ath79_register_gpio_keys_polled(-1, UBNT_XM_KEYS_POLL_INTERVAL,
+                                        ARRAY_SIZE(ubnt_xm_gpio_keys),
+                                        ubnt_xm_gpio_keys);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_AIRROUTER, "UBNT-AR", "Ubiquiti AirRouter",
+	     ubnt_airrouter_setup);
+
+static struct gpio_led ubnt_unifi_leds_gpio[] __initdata = {
+	{
+		.name		= "ubnt:orange:dome",
+		.gpio		= 1,
+		.active_low	= 0,
+	}, {
+		.name		= "ubnt:green:dome",
+		.gpio		= 0,
+		.active_low	= 0,
+	}
+};
+
+static struct gpio_led ubnt_unifi_outdoor_leds_gpio[] __initdata = {
+	{
+		.name		= "ubnt:orange:front",
+		.gpio		= 1,
+		.active_low	= 0,
+	}, {
+		.name		= "ubnt:green:front",
+		.gpio		= 0,
+		.active_low	= 0,
+	}
+};
+
+static struct gpio_led ubnt_unifi_outdoor_plus_leds_gpio[] __initdata = {
+	{
+		.name		= "ubnt:white:front",
+		.gpio		= 1,
+		.active_low	= 0,
+	}, {
+		.name		= "ubnt:blue:front",
+		.gpio		= 0,
+		.active_low	= 0,
+	}
+};
+
+
+static void __init ubnt_unifi_setup(void)
+{
+	u8 *mac = (u8 *) KSEG1ADDR(0x1fff0000);
+	u8 *ee = (u8 *) KSEG1ADDR(0x1fff1000);
+
+	ath79_register_m25p80(NULL);
+
+	ath79_register_mdio(0, ~UBNT_M_WAN_PHYMASK);
+
+	ath79_init_mac(ath79_eth0_data.mac_addr, mac, 0);
+	ath79_register_eth(0);
+
+	ap91_pci_init(ee, NULL);
+
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_unifi_leds_gpio),
+				 ubnt_unifi_leds_gpio);
+
+	ath79_register_gpio_keys_polled(-1, UBNT_XM_KEYS_POLL_INTERVAL,
+                                        ARRAY_SIZE(ubnt_xm_gpio_keys),
+                                        ubnt_xm_gpio_keys);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_UNIFI, "UBNT-UF", "Ubiquiti UniFi",
+	     ubnt_unifi_setup);
+
+
+#define UBNT_UNIFIOD_PRI_PHYMASK	BIT(4)
+#define UBNT_UNIFIOD_2ND_PHYMASK	(BIT(0) | BIT(1) | BIT(2) | BIT(3))
+
+static void __init ubnt_unifi_outdoor_setup(void)
+{
+	u8 *mac1 = (u8 *) KSEG1ADDR(0x1fff0000);
+	u8 *mac2 = (u8 *) KSEG1ADDR(0x1fff0000 + ETH_ALEN);
+	u8 *ee = (u8 *) KSEG1ADDR(0x1fff1000);
+
+	ath79_register_m25p80(NULL);
+
+	ath79_register_mdio(0, ~(UBNT_UNIFIOD_PRI_PHYMASK |
+				 UBNT_UNIFIOD_2ND_PHYMASK));
+
+	ath79_init_mac(ath79_eth0_data.mac_addr, mac1, 0);
+	ath79_init_mac(ath79_eth1_data.mac_addr, mac2, 0);
+	ath79_register_eth(0);
+	ath79_register_eth(1);
+
+	ap91_pci_init(ee, NULL);
+
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_unifi_outdoor_leds_gpio),
+				 ubnt_unifi_outdoor_leds_gpio);
+
+	ath79_register_gpio_keys_polled(-1, UBNT_XM_KEYS_POLL_INTERVAL,
+                                        ARRAY_SIZE(ubnt_xm_gpio_keys),
+                                        ubnt_xm_gpio_keys);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_UNIFI_OUTDOOR, "UBNT-U20",
+	     "Ubiquiti UniFiAP Outdoor",
+	     ubnt_unifi_outdoor_setup);
+
+
+static void __init ubnt_unifi_outdoor_plus_setup(void)
+{
+	u8 *mac1 = (u8 *) KSEG1ADDR(0x1fff0000);
+	u8 *mac2 = (u8 *) KSEG1ADDR(0x1fff0000 + ETH_ALEN);
+	u8 *ee = (u8 *) KSEG1ADDR(0x1fff1000);
+
+	ath79_register_m25p80(NULL);
+
+	ath79_register_mdio(0, ~(UBNT_UNIFIOD_PRI_PHYMASK |
+				 UBNT_UNIFIOD_2ND_PHYMASK));
+
+	ath79_init_mac(ath79_eth0_data.mac_addr, mac1, 0);
+	ath79_init_mac(ath79_eth1_data.mac_addr, mac2, 0);
+	ath79_register_eth(0);
+	ath79_register_eth(1);
+
+	ap91_pci_init(ee, NULL);
+
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_unifi_outdoor_plus_leds_gpio),
+				 ubnt_unifi_outdoor_plus_leds_gpio);
+
+	ath79_register_gpio_keys_polled(-1, UBNT_XM_KEYS_POLL_INTERVAL,
+                                        ARRAY_SIZE(ubnt_xm_gpio_keys),
+                                        ubnt_xm_gpio_keys);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_UNIFI_OUTDOOR_PLUS, "UBNT-UOP",
+	     "Ubiquiti UniFiAP Outdoor+",
+	     ubnt_unifi_outdoor_plus_setup);
+
+
+static struct gpio_led ubnt_uap_pro_gpio_leds[] __initdata = {
+	{
+		.name		= "ubnt:white:dome",
+		.gpio		= 12,
+	}, {
+		.name		= "ubnt:blue:dome",
+		.gpio		= 13,
+	}
+};
+
+static struct gpio_keys_button uap_pro_gpio_keys[] __initdata = {
+	{
+		.desc			= "reset",
+		.type			= EV_KEY,
+		.code			= KEY_RESTART,
+		.debounce_interval	= UBNT_XM_KEYS_DEBOUNCE_INTERVAL,
+		.gpio			= 17,
+		.active_low		= 1,
+	}
+};
+
+static struct ar8327_pad_cfg uap_pro_ar8327_pad0_cfg = {
+	.mode = AR8327_PAD_MAC_RGMII,
+	.txclk_delay_en = true,
+	.rxclk_delay_en = true,
+	.txclk_delay_sel = AR8327_CLK_DELAY_SEL1,
+	.rxclk_delay_sel = AR8327_CLK_DELAY_SEL2,
+};
+
+static struct ar8327_platform_data uap_pro_ar8327_data = {
+	.pad0_cfg = &uap_pro_ar8327_pad0_cfg,
+	.port0_cfg = {
+		.force_link = 1,
+		.speed = AR8327_PORT_SPEED_1000,
+		.duplex = 1,
+		.txpause = 1,
+		.rxpause = 1,
+	},
+};
+
+static struct mdio_board_info uap_pro_mdio0_info[] = {
+	{
+		.bus_id = "ag71xx-mdio.0",
+		.phy_addr = 0,
+		.platform_data = &uap_pro_ar8327_data,
+	},
+};
+
+#define UAP_PRO_MAC0_OFFSET		0x0000
+#define UAP_PRO_MAC1_OFFSET		0x0006
+#define UAP_PRO_WMAC_CALDATA_OFFSET	0x1000
+#define UAP_PRO_PCI_CALDATA_OFFSET	0x5000
+
+static void __init ubnt_uap_pro_setup(void)
+{
+	u8 *eeprom = (u8 *) KSEG1ADDR(0x1fff0000);
+
+	ath79_register_m25p80(NULL);
+
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_uap_pro_gpio_leds),
+				 ubnt_uap_pro_gpio_leds);
+	ath79_register_gpio_keys_polled(-1, UBNT_XM_KEYS_POLL_INTERVAL,
+                                        ARRAY_SIZE(uap_pro_gpio_keys),
+                                        uap_pro_gpio_keys);
+
+	ath79_register_wmac(eeprom + UAP_PRO_WMAC_CALDATA_OFFSET, NULL);
+	ap91_pci_init(eeprom + UAP_PRO_PCI_CALDATA_OFFSET, NULL);
+
+	ath79_register_mdio(0, 0x0);
+	mdiobus_register_board_info(uap_pro_mdio0_info,
+				    ARRAY_SIZE(uap_pro_mdio0_info));
+
+	ath79_setup_ar934x_eth_cfg(AR934X_ETH_CFG_RGMII_GMAC0);
+	ath79_init_mac(ath79_eth0_data.mac_addr,
+		       eeprom + UAP_PRO_MAC0_OFFSET, 0);
+
+	/* GMAC0 is connected to an AR8327 switch */
+	ath79_eth0_data.phy_if_mode = PHY_INTERFACE_MODE_RGMII;
+	ath79_eth0_data.phy_mask = BIT(0);
+	ath79_eth0_data.mii_bus_dev = &ath79_mdio0_device.dev;
+	ath79_eth0_pll_data.pll_1000 = 0x06000000;
+	ath79_register_eth(0);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_UAP_PRO, "UAP-PRO", "Ubiquiti UniFi AP Pro",
+	     ubnt_uap_pro_setup);
+
+#define UBNT_XW_GPIO_LED_L1		11
+#define UBNT_XW_GPIO_LED_L2		16
+#define UBNT_XW_GPIO_LED_L3		13
+#define UBNT_XW_GPIO_LED_L4		14
+
+static struct gpio_led ubnt_xw_leds_gpio[] __initdata = {
+	{
+		.name		= "ubnt:red:link1",
+		.gpio		= UBNT_XW_GPIO_LED_L1,
+		.active_low	= 1,
+	}, {
+		.name		= "ubnt:orange:link2",
+		.gpio		= UBNT_XW_GPIO_LED_L2,
+		.active_low	= 1,
+	}, {
+		.name		= "ubnt:green:link3",
+		.gpio		= UBNT_XW_GPIO_LED_L3,
+		.active_low	= 1,
+	}, {
+		.name		= "ubnt:green:link4",
+		.gpio		= UBNT_XW_GPIO_LED_L4,
+		.active_low	= 1,
+	},
+};
+
+static void __init ubnt_xw_init(void)
+{
+	u8 *eeprom = (u8 *) KSEG1ADDR(0x1fff0000);
+
+	ath79_register_m25p80(NULL);
+
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_xw_leds_gpio),
+				 ubnt_xw_leds_gpio);
+	ath79_register_gpio_keys_polled(-1, UBNT_XM_KEYS_POLL_INTERVAL,
+                                        ARRAY_SIZE(ubnt_xm_gpio_keys),
+                                        ubnt_xm_gpio_keys);
+
+	ath79_register_wmac(eeprom + UAP_PRO_WMAC_CALDATA_OFFSET, NULL);
+	ap91_pci_init(eeprom + UAP_PRO_PCI_CALDATA_OFFSET, NULL);
+
+
+	ath79_setup_ar934x_eth_cfg(AR934X_ETH_CFG_MII_GMAC0 | AR934X_ETH_CFG_MII_GMAC0_SLAVE);
+	ath79_init_mac(ath79_eth0_data.mac_addr,
+		       eeprom + UAP_PRO_MAC0_OFFSET, 0);
+
+	ath79_eth0_data.phy_if_mode = PHY_INTERFACE_MODE_MII;
+	ath79_eth0_data.mii_bus_dev = &ath79_mdio0_device.dev;
+}
+
+static void __init ubnt_nano_m_xw_setup(void)
+{
+	ubnt_xw_init();
+
+	/* GMAC0 is connected to an AR8326 switch */
+	ath79_register_mdio(0, ~(BIT(0) | BIT(1) | BIT(5)));
+	ath79_eth0_data.phy_mask = (BIT(0) | BIT(1) | BIT(5));
+	ath79_eth0_data.speed = SPEED_100;
+	ath79_eth0_data.duplex = DUPLEX_FULL;
+	ath79_register_eth(0);
+}
+
+static void __init ubnt_loco_m_xw_setup(void)
+{
+	ubnt_xw_init();
+
+	ath79_register_mdio(0, ~BIT(1));
+	ath79_eth0_data.phy_mask = BIT(1);
+	ath79_register_eth(0);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_NANO_M_XW, "UBNT-NM-XW", "Ubiquiti Nanostation M XW",
+	     ubnt_nano_m_xw_setup);
+
+MIPS_MACHINE(ATH79_MACH_UBNT_LOCO_M_XW, "UBNT-LOCO-XW", "Ubiquiti Loco M XW",
+	     ubnt_loco_m_xw_setup);
+
+static struct gpio_led ubnt_airgateway_gpio_leds[] __initdata = {
+	{
+		.name	   = "ubnt:blue:wlan",
+		.gpio	   = 0,
+	}, {
+		.name	   = "ubnt:white:status",
+		.gpio	   = 1,
+	},
+};
+
+static struct gpio_keys_button airgateway_gpio_keys[] __initdata = {
+	{
+		.desc		= "reset",
+		.type		= EV_KEY,
+		.code		= KEY_RESTART,
+		.debounce_interval	= UBNT_XM_KEYS_DEBOUNCE_INTERVAL,
+		.gpio		= 12,
+		.active_low	= 1,
+	}
+};
+
+static void __init ubnt_airgateway_setup(void)
+{
+	u32 t;
+	u8 *mac0 = (u8 *) KSEG1ADDR(0x1fff0000);
+	u8 *mac1 = (u8 *) KSEG1ADDR(0x1fff0000 + ETH_ALEN);
+	u8 *ee = (u8 *) KSEG1ADDR(0x1fff1000);
+
+
+	ath79_gpio_function_disable(AR933X_GPIO_FUNC_ETH_SWITCH_LED0_EN |
+				     AR933X_GPIO_FUNC_ETH_SWITCH_LED1_EN |
+				     AR933X_GPIO_FUNC_ETH_SWITCH_LED2_EN |
+				     AR933X_GPIO_FUNC_ETH_SWITCH_LED3_EN |
+				     AR933X_GPIO_FUNC_ETH_SWITCH_LED4_EN);
+
+	t = ath79_reset_rr(AR933X_RESET_REG_BOOTSTRAP);
+	t |= AR933X_BOOTSTRAP_MDIO_GPIO_EN;
+	ath79_reset_wr(AR933X_RESET_REG_BOOTSTRAP, t);
+
+	ath79_register_m25p80(NULL);
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_airgateway_gpio_leds),
+				 ubnt_airgateway_gpio_leds);
+
+	ath79_register_gpio_keys_polled(-1, UBNT_XM_KEYS_POLL_INTERVAL,
+					ARRAY_SIZE(airgateway_gpio_keys),
+					airgateway_gpio_keys);
+
+	ath79_init_mac(ath79_eth1_data.mac_addr, mac0, 0);
+	ath79_init_mac(ath79_eth0_data.mac_addr, mac1, 0);
+
+	ath79_register_mdio(0, 0x0);
+
+	ath79_register_eth(1);
+	ath79_register_eth(0);
+
+	ath79_register_wmac(ee, NULL);
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_AIRGW, "UBNT-AGW", "Ubiquiti AirGateway",
+	     ubnt_airgateway_setup);
+
--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -68,12 +68,16 @@ config ATH79_MACH_PB44
 	  Atheros PB44 reference board.
 
 config ATH79_MACH_UBNT_XM
-	bool "Ubiquiti Networks XM (rev 1.0) board"
+	bool "Ubiquiti Networks XM/UniFi boards"
 	select SOC_AR724X
+	select SOC_AR934X
 	select ATH79_DEV_AP9X_PCI if PCI
+	select ATH79_DEV_ETH
 	select ATH79_DEV_GPIO_BUTTONS
 	select ATH79_DEV_LEDS_GPIO
 	select ATH79_DEV_M25P80
+	select ATH79_DEV_USB
+	select ATH79_DEV_WMAC
 	help
 	  Say 'Y' here if you want your kernel to support the
 	  Ubiquiti Networks XM (rev 1.0) board.
--- a/arch/mips/ath79/machtypes.h
+++ b/arch/mips/ath79/machtypes.h
@@ -22,6 +22,13 @@ enum ath79_mach_type {
 	ATH79_MACH_AP81,		/* Atheros AP81 reference board */
 	ATH79_MACH_DB120,		/* Atheros DB120 reference board */
 	ATH79_MACH_PB44,		/* Atheros PB44 reference board */
+	ATH79_MACH_UBNT_AIRROUTER,	/* Ubiquiti AirRouter */
+	ATH79_MACH_UBNT_BULLET_M,	/* Ubiquiti Bullet M */
+	ATH79_MACH_UBNT_NANO_M, 	/* Ubiquiti NanoStation M */
+	ATH79_MACH_UBNT_ROCKET_M,	/* Ubiquiti Rocket M */
+	ATH79_MACH_UBNT_UAP_PRO,	/* Ubiquiti UniFi AP Pro */
+	ATH79_MACH_UBNT_UNIFI, 		/* Ubiquiti Unifi */
+	ATH79_MACH_UBNT_UNIFI_OUTDOOR,	/* Ubiquiti UnifiAP Outdoor */
 	ATH79_MACH_UBNT_XM,		/* Ubiquiti Networks XM board rev 1.0 */
 };
 
