From dd7733da69f198f576d7f52f6bc5a860fe24930d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Thu, 4 Dec 2014 10:24:02 +0100
Subject: [PATCH] ARM: BCM5301X: Add DT for Buffalo WZR-600DHP2
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 arch/arm/boot/dts/Makefile                         |  3 +-
 arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts | 57 ++++++++++++++++++++++
 2 files changed, 59 insertions(+), 1 deletion(-)
 create mode 100644 arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -58,7 +58,8 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm4708-buffalo-wzr-1750dhp.dtb \
 	bcm4708-netgear-r6250.dtb \
 	bcm4708-netgear-r6300-v2.dtb \
-	bcm47081-asus-rt-n18u.dtb
+	bcm47081-asus-rt-n18u.dtb \
+	bcm47081-buffalo-wzr-600dhp2.dtb
 dtb-$(CONFIG_ARCH_BCM_63XX) += bcm963138dvt.dtb
 dtb-$(CONFIG_ARCH_BCM_MOBILE) += bcm28155-ap.dtb \
 	bcm21664-garnet.dtb
--- /dev/null
+++ b/arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts
@@ -0,0 +1,57 @@
+/*
+ * Broadcom BCM470X / BCM5301X ARM platform code.
+ * DTS for Buffalo WZR-600DHP2
+ *
+ * Copyright (C) 2014 Rafał Miłecki <zajec5@gmail.com>
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+
+/dts-v1/;
+
+#include "bcm47081.dtsi"
+
+/ {
+	compatible = "buffalo,wzr-600dhp2", "brcm,bcm47081", "brcm,bcm4708";
+	model = "Buffalo WZR-600DHP2 (BCM47081)";
+
+	chosen {
+		bootargs = "console=ttyS0,115200";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000>;
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		poll-interval = <200>;
+
+		aoss {
+			label = "AOSS";
+			linux,code = <KEY_WPS_BUTTON>;
+			gpios = <&chipcommon 9 GPIO_ACTIVE_LOW>;
+		};
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
+		};
+
+		/* Switch device mode? */
+		mode {
+			label = "Mode";
+			linux,code = <KEY_SETUP>;
+			gpios = <&chipcommon 14 GPIO_ACTIVE_LOW>;
+		};
+
+		eject {
+			label = "USB eject";
+			linux,code = <KEY_EJECTCD>;
+			gpios = <&chipcommon 15 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
