From 8a0803979163c647736cb234ee1620c049c4915c Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Mon, 1 Dec 2014 00:20:07 +0100
Subject: [PATCH 5/5] MIPS: BCM63XX: register interrupt controllers through DT

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/bcm63xx/irq.c |   12 +++++++++++-
 1 file changed, 11 insertions(+), 1 deletion(-)

--- a/arch/mips/bcm63xx/irq.c
+++ b/arch/mips/bcm63xx/irq.c
@@ -15,6 +15,8 @@
 #include <linux/irqchip.h>
 #include <linux/irqchip/irq-bcm6345-ext.h>
 #include <linux/irqchip/irq-bcm6345-periph.h>
+#include <linux/of.h>
+#include <linux/of_fdt.h>
 #include <asm/irq_cpu.h>
 #include <asm/mipsregs.h>
 #include <bcm63xx_cpu.h>
@@ -190,7 +192,15 @@ static void bcm63xx_init_irq(void)
 				      ext_shift);
 }
 
+OF_DECLARE_2(irqchip, mips_cpu_intc, "mti,cpu-interrupt-controller",
+	     mips_cpu_irq_of_init);
+
 void __init arch_init_irq(void)
 {
-	bcm63xx_init_irq();
+#ifdef CONFIG_OF
+	if (initial_boot_params)
+		irqchip_init();
+	else
+#endif
+		bcm63xx_init_irq();
 }
