#!/bin/sh

. /lib/functions/uci-defaults-new.sh
. /lib/oxnas.sh

board=$(oxnas_board_name)
board_config_update

case $board in
	stg-212)
		ucidef_set_led_default "power" "power" "zyxel:blue:status" "1"
		ucidef_set_led_usbdev "usb" "USB" "$1" "1-1"
		;;
	kd20)
		ucidef_set_led_default "power" "power" "kd20:blue:status" "1"
		;;
	pogoplugpro | pogoplugv3)
		ucidef_set_led_default "power" "power" "pogoplug:blue:internal" "1"
		;;

esac

board_config_flush

exit 0
