From 709288ac793d8a070f33c36e76ca03281fa6b417 Mon Sep 17 00:00:00 2001
From: Daniel Matuschek <info@crazy-audio.com>
Date: Mon, 4 Aug 2014 11:09:58 +0200
Subject: [PATCH 061/114] Added driver for HiFiBerry Amp amplifier add-on board

The driver contains a low-level hardware driver for the TAS5713 and the
drivers for the Raspberry Pi I2S subsystem.
---
 arch/arm/configs/bcmrpi_defconfig |   1 +
 arch/arm/mach-bcm2708/bcm2708.c   |  20 +++
 sound/soc/bcm/Kconfig             |   7 +
 sound/soc/bcm/Makefile            |   2 +
 sound/soc/bcm/hifiberry_amp.c     | 106 +++++++++++
 sound/soc/codecs/Kconfig          |   4 +
 sound/soc/codecs/Makefile         |   2 +
 sound/soc/codecs/tas5713.c        | 362 ++++++++++++++++++++++++++++++++++++++
 sound/soc/codecs/tas5713.h        | 210 ++++++++++++++++++++++
 9 files changed, 714 insertions(+)
 create mode 100644 sound/soc/bcm/hifiberry_amp.c
 create mode 100644 sound/soc/codecs/tas5713.c
 create mode 100644 sound/soc/codecs/tas5713.h

--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -758,6 +758,7 @@ CONFIG_SND_BCM2708_SOC_I2S=m
 CONFIG_SND_BCM2708_SOC_HIFIBERRY_DAC=m
 CONFIG_SND_BCM2708_SOC_HIFIBERRY_DACPLUS=m
 CONFIG_SND_BCM2708_SOC_HIFIBERRY_DIGI=m
+CONFIG_SND_BCM2708_SOC_HIFIBERRY_AMP=m
 CONFIG_SND_BCM2708_SOC_RPI_DAC=m
 CONFIG_SND_BCM2708_SOC_IQAUDIO_DAC=m
 CONFIG_SND_SIMPLE_CARD=m
--- a/arch/arm/mach-bcm2708/bcm2708.c
+++ b/arch/arm/mach-bcm2708/bcm2708.c
@@ -674,6 +674,20 @@ static struct i2c_board_info __initdata
 
 #endif
 
+#if defined(CONFIG_SND_BCM2708_SOC_HIFIBERRY_AMP) || defined(CONFIG_SND_BCM2708_SOC_HIFIBERRY_AMP_MODULE)
+static struct platform_device snd_hifiberry_amp_device = {
+        .name = "snd-hifiberry-amp",
+        .id = 0,
+        .num_resources = 0,
+};
+
+static struct i2c_board_info __initdata snd_tas5713_i2c_devices[] = {
+        {
+                I2C_BOARD_INFO("tas5713", 0x1b)
+        },
+};
+#endif
+
 #if defined(CONFIG_SND_BCM2708_SOC_RPI_DAC) || defined(CONFIG_SND_BCM2708_SOC_RPI_DAC_MODULE)
 static struct platform_device snd_rpi_dac_device = {
         .name = "snd-rpi-dac",
@@ -869,6 +883,12 @@ void __init bcm2708_init(void)
         i2c_register_board_info(1, snd_wm8804_i2c_devices, ARRAY_SIZE(snd_wm8804_i2c_devices));
 #endif
 
+#if defined(CONFIG_SND_BCM2708_SOC_HIFIBERRY_AMP) || defined(CONFIG_SND_BCM2708_SOC_HIFIBERRY_AMP_MODULE)
+        bcm_register_device(&snd_hifiberry_amp_device);
+        i2c_register_board_info(1, snd_tas5713_i2c_devices, ARRAY_SIZE(snd_tas5713_i2c_devices));
+#endif
+
+
 #if defined(CONFIG_SND_BCM2708_SOC_RPI_DAC) || defined(CONFIG_SND_BCM2708_SOC_RPI_DAC_MODULE)
         bcm_register_device(&snd_rpi_dac_device);
         bcm_register_device(&snd_pcm1794a_codec_device);
--- a/sound/soc/bcm/Kconfig
+++ b/sound/soc/bcm/Kconfig
@@ -40,6 +40,13 @@ config SND_BCM2708_SOC_HIFIBERRY_DIGI
         help
          Say Y or M if you want to add support for HifiBerry Digi S/PDIF output board.
 
+config SND_BCM2708_SOC_HIFIBERRY_AMP
+        tristate "Support for the HifiBerry Amp"
+        depends on SND_BCM2708_SOC_I2S
+        select SND_SOC_TAS5713
+        help
+         Say Y or M if you want to add support for the HifiBerry Amp amplifier board.
+
 config SND_BCM2708_SOC_RPI_DAC
         tristate "Support for RPi-DAC"
         depends on SND_BCM2708_SOC_I2S
--- a/sound/soc/bcm/Makefile
+++ b/sound/soc/bcm/Makefile
@@ -12,11 +12,13 @@ obj-$(CONFIG_SND_BCM2708_SOC_I2S) += snd
 snd-soc-hifiberry-dac-objs := hifiberry_dac.o
 snd-soc-hifiberry-dacplus-objs := hifiberry_dacplus.o
 snd-soc-hifiberry-digi-objs := hifiberry_digi.o
+snd-soc-hifiberry-amp-objs := hifiberry_amp.o
 snd-soc-rpi-dac-objs := rpi-dac.o
 snd-soc-iqaudio-dac-objs := iqaudio-dac.o
 
 obj-$(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DAC) += snd-soc-hifiberry-dac.o
 obj-$(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DACPLUS) += snd-soc-hifiberry-dacplus.o
 obj-$(CONFIG_SND_BCM2708_SOC_HIFIBERRY_DIGI) += snd-soc-hifiberry-digi.o
+obj-$(CONFIG_SND_BCM2708_SOC_HIFIBERRY_AMP) += snd-soc-hifiberry-amp.o
 obj-$(CONFIG_SND_BCM2708_SOC_RPI_DAC) += snd-soc-rpi-dac.o
 obj-$(CONFIG_SND_BCM2708_SOC_IQAUDIO_DAC) += snd-soc-iqaudio-dac.o
--- /dev/null
+++ b/sound/soc/bcm/hifiberry_amp.c
@@ -0,0 +1,106 @@
+/*
+ * ASoC Driver for HifiBerry AMP
+ *
+ * Author:	Sebastian Eickhoff <basti.eickhoff@googlemail.com>
+ *		Copyright 2014
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ */
+
+#include <linux/module.h>
+#include <linux/platform_device.h>
+
+#include <sound/core.h>
+#include <sound/pcm.h>
+#include <sound/pcm_params.h>
+#include <sound/soc.h>
+#include <sound/jack.h>
+
+static int snd_rpi_hifiberry_amp_init(struct snd_soc_pcm_runtime *rtd)
+{
+	// ToDo: init of the dsp-registers.
+	return 0;
+}
+
+static int snd_rpi_hifiberry_amp_hw_params( struct snd_pcm_substream *substream,
+				       struct snd_pcm_hw_params *params )
+{
+	struct snd_soc_pcm_runtime *rtd = substream->private_data;
+	struct snd_soc_dai *cpu_dai = rtd->cpu_dai;
+
+	return snd_soc_dai_set_bclk_ratio(cpu_dai, 64);
+}
+
+static struct snd_soc_ops snd_rpi_hifiberry_amp_ops = {
+	.hw_params = snd_rpi_hifiberry_amp_hw_params,
+};
+
+static struct snd_soc_dai_link snd_rpi_hifiberry_amp_dai[] = {
+    {
+		.name			= "HifiBerry AMP",
+		.stream_name	= "HifiBerry AMP HiFi",
+		.cpu_dai_name	= "bcm2708-i2s.0",
+		.codec_dai_name	= "tas5713-hifi",
+		.platform_name	= "bcm2708-i2s.0",
+		.codec_name		= "tas5713.1-001b",
+		.dai_fmt		= SND_SOC_DAIFMT_I2S |
+						  SND_SOC_DAIFMT_NB_NF |
+						  SND_SOC_DAIFMT_CBS_CFS,
+		.ops			= &snd_rpi_hifiberry_amp_ops,
+		.init			= snd_rpi_hifiberry_amp_init,
+	},
+};
+
+
+static struct snd_soc_card snd_rpi_hifiberry_amp = {
+	.name         = "snd_rpi_hifiberry_amp",
+	.dai_link     = snd_rpi_hifiberry_amp_dai,
+	.num_links    = ARRAY_SIZE(snd_rpi_hifiberry_amp_dai),
+};
+
+
+static int snd_rpi_hifiberry_amp_probe(struct platform_device *pdev)
+{
+	int ret = 0;
+
+	snd_rpi_hifiberry_amp.dev = &pdev->dev;
+
+	ret = snd_soc_register_card(&snd_rpi_hifiberry_amp);
+
+	if (ret != 0) {
+		dev_err(&pdev->dev, "snd_soc_register_card() failed: %d\n", ret);
+	}
+
+	return ret;
+}
+
+
+static int snd_rpi_hifiberry_amp_remove(struct platform_device *pdev)
+{
+	return snd_soc_unregister_card(&snd_rpi_hifiberry_amp);
+}
+
+
+static struct platform_driver snd_rpi_hifiberry_amp_driver = {
+        .driver = {
+                .name   = "snd-hifiberry-amp",
+                .owner  = THIS_MODULE,
+        },
+        .probe          = snd_rpi_hifiberry_amp_probe,
+        .remove         = snd_rpi_hifiberry_amp_remove,
+};
+
+
+module_platform_driver(snd_rpi_hifiberry_amp_driver);
+
+
+MODULE_AUTHOR("Sebastian Eickhoff <basti.eickhoff@googlemail.com>");
+MODULE_DESCRIPTION("ASoC driver for HiFiBerry-AMP");
+MODULE_LICENSE("GPL v2");
--- a/sound/soc/codecs/Kconfig
+++ b/sound/soc/codecs/Kconfig
@@ -105,6 +105,7 @@ config SND_SOC_ALL_CODECS
 	select SND_SOC_TAS5086 if I2C
 	select SND_SOC_TLV320AIC23_I2C if I2C
 	select SND_SOC_TLV320AIC23_SPI if SPI_MASTER
+	select SND_SOC_TAS5713 if I2C
 	select SND_SOC_TLV320AIC26 if SPI_MASTER
 	select SND_SOC_TLV320AIC31XX if I2C
 	select SND_SOC_TLV320AIC32X4 if I2C
@@ -585,6 +586,9 @@ config SND_SOC_TAS5086
 	tristate "Texas Instruments TAS5086 speaker amplifier"
 	depends on I2C
 
+config SND_SOC_TAS5713
+	tristate
+
 config SND_SOC_TLV320AIC23
 	tristate
 
--- a/sound/soc/codecs/Makefile
+++ b/sound/soc/codecs/Makefile
@@ -103,6 +103,7 @@ snd-soc-sta350-objs := sta350.o
 snd-soc-sta529-objs := sta529.o
 snd-soc-stac9766-objs := stac9766.o
 snd-soc-tas5086-objs := tas5086.o
+snd-soc-tas5713-objs := tas5713.o
 snd-soc-tlv320aic23-objs := tlv320aic23.o
 snd-soc-tlv320aic23-i2c-objs := tlv320aic23-i2c.o
 snd-soc-tlv320aic23-spi-objs := tlv320aic23-spi.o
@@ -278,6 +279,7 @@ obj-$(CONFIG_SND_SOC_STA529)   += snd-so
 obj-$(CONFIG_SND_SOC_STAC9766)	+= snd-soc-stac9766.o
 obj-$(CONFIG_SND_SOC_TAS2552)	+= snd-soc-tas2552.o
 obj-$(CONFIG_SND_SOC_TAS5086)	+= snd-soc-tas5086.o
+obj-$(CONFIG_SND_SOC_TAS5713)	+= snd-soc-tas5713.o
 obj-$(CONFIG_SND_SOC_TLV320AIC23)	+= snd-soc-tlv320aic23.o
 obj-$(CONFIG_SND_SOC_TLV320AIC23_I2C)	+= snd-soc-tlv320aic23-i2c.o
 obj-$(CONFIG_SND_SOC_TLV320AIC23_SPI)	+= snd-soc-tlv320aic23-spi.o
--- /dev/null
+++ b/sound/soc/codecs/tas5713.c
@@ -0,0 +1,362 @@
+/*
+ * ASoC Driver for TAS5713
+ *
+ * Author:	Sebastian Eickhoff <basti.eickhoff@googlemail.com>
+ *		Copyright 2014
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ */
+
+#include <linux/module.h>
+#include <linux/moduleparam.h>
+#include <linux/init.h>
+#include <linux/delay.h>
+#include <linux/pm.h>
+#include <linux/i2c.h>
+#include <linux/of_device.h>
+#include <linux/spi/spi.h>
+#include <linux/regmap.h>
+#include <linux/regulator/consumer.h>
+#include <linux/slab.h>
+#include <sound/core.h>
+#include <sound/pcm.h>
+#include <sound/pcm_params.h>
+#include <sound/soc.h>
+#include <sound/initval.h>
+#include <sound/tlv.h>
+
+#include <linux/kernel.h>
+#include <linux/string.h>
+#include <linux/fs.h>
+#include <asm/uaccess.h>
+
+#include "tas5713.h"
+
+
+static struct i2c_client *i2c;
+
+struct tas5713_priv {
+	struct regmap *regmap;
+	int mclk_div;
+	struct snd_soc_codec *codec;
+};
+
+static struct tas5713_priv *priv_data;
+
+
+
+
+/*
+ *    _   _    ___   _      ___         _           _
+ *   /_\ | |  / __| /_\    / __|___ _ _| |_ _ _ ___| |___
+ *  / _ \| |__\__ \/ _ \  | (__/ _ \ ' \  _| '_/ _ \ (_-<
+ * /_/ \_\____|___/_/ \_\  \___\___/_||_\__|_| \___/_/__/
+ *
+ */
+
+static const DECLARE_TLV_DB_SCALE(tas5713_vol_tlv, -10000, 50, 1);
+
+
+static const struct snd_kcontrol_new tas5713_snd_controls[] = {
+	SOC_SINGLE_TLV  ("Master"    , TAS5713_VOL_MASTER, 0, 248, 1, tas5713_vol_tlv),
+	SOC_DOUBLE_R_TLV("Channels"  , TAS5713_VOL_CH1, TAS5713_VOL_CH2, 0, 248, 1, tas5713_vol_tlv)
+};
+
+
+
+
+/*
+ *  __  __         _    _            ___      _
+ * |  \/  |__ _ __| |_ (_)_ _  ___  |   \ _ _(_)_ _____ _ _
+ * | |\/| / _` / _| ' \| | ' \/ -_) | |) | '_| \ V / -_) '_|
+ * |_|  |_\__,_\__|_||_|_|_||_\___| |___/|_| |_|\_/\___|_|
+ *
+ */
+
+static int tas5713_hw_params(struct snd_pcm_substream *substream,
+			    struct snd_pcm_hw_params *params,
+			    struct snd_soc_dai *dai)
+{
+	u16 blen = 0x00;
+
+	struct snd_soc_codec *codec;
+	codec = dai->codec;
+	priv_data->codec = dai->codec;
+
+	switch (params_format(params)) {
+	case SNDRV_PCM_FORMAT_S16_LE:
+		blen = 0x03;
+		break;
+	case SNDRV_PCM_FORMAT_S20_3LE:
+		blen = 0x1;
+		break;
+	case SNDRV_PCM_FORMAT_S24_LE:
+		blen = 0x04;
+		break;
+	case SNDRV_PCM_FORMAT_S32_LE:
+		blen = 0x05;
+		break;
+	default:
+		dev_err(dai->dev, "Unsupported word length: %u\n",
+			params_format(params));
+		return -EINVAL;
+	}
+
+	// set word length
+	snd_soc_update_bits(codec, TAS5713_SERIAL_DATA_INTERFACE, 0x7, blen);
+
+	return 0;
+}
+
+
+static int tas5713_mute_stream(struct snd_soc_dai *dai, int mute, int stream)
+{
+	unsigned int val = 0;
+
+	struct tas5713_priv *tas5713;
+	struct snd_soc_codec *codec = dai->codec;
+	tas5713 = snd_soc_codec_get_drvdata(codec);
+
+	if (mute) {
+		val = TAS5713_SOFT_MUTE_ALL;
+	}
+
+	return regmap_write(tas5713->regmap, TAS5713_SOFT_MUTE, val);
+}
+
+
+static const struct snd_soc_dai_ops tas5713_dai_ops = {
+	.hw_params 		= tas5713_hw_params,
+	.mute_stream	= tas5713_mute_stream,
+};
+
+
+static struct snd_soc_dai_driver tas5713_dai = {
+	.name		= "tas5713-hifi",
+	.playback 	= {
+		.stream_name	= "Playback",
+		.channels_min	= 2,
+		.channels_max	= 2,
+		.rates		    = SNDRV_PCM_RATE_8000_48000,
+		.formats	    = (SNDRV_PCM_FMTBIT_S16_LE | SNDRV_PCM_FMTBIT_S24_LE | SNDRV_PCM_FMTBIT_S32_LE ),
+	},
+	.ops        = &tas5713_dai_ops,
+};
+
+
+
+
+/*
+ *   ___         _          ___      _
+ *  / __|___  __| |___ __  |   \ _ _(_)_ _____ _ _
+ * | (__/ _ \/ _` / -_) _| | |) | '_| \ V / -_) '_|
+ *  \___\___/\__,_\___\__| |___/|_| |_|\_/\___|_|
+ *
+ */
+
+static int tas5713_remove(struct snd_soc_codec *codec)
+{
+	struct tas5713_priv *tas5713;
+
+	tas5713 = snd_soc_codec_get_drvdata(codec);
+
+	return 0;
+}
+
+
+static int tas5713_probe(struct snd_soc_codec *codec)
+{
+	struct tas5713_priv *tas5713;
+	int i, ret;
+
+	i2c = container_of(codec->dev, struct i2c_client, dev);
+
+	tas5713 = snd_soc_codec_get_drvdata(codec);
+
+	// Reset error
+	ret = snd_soc_write(codec, TAS5713_ERROR_STATUS, 0x00);
+
+	// Trim oscillator
+    ret = snd_soc_write(codec, TAS5713_OSC_TRIM, 0x00);
+	msleep(1000);
+
+	// Reset error
+	ret = snd_soc_write(codec, TAS5713_ERROR_STATUS, 0x00);
+
+	// Clock mode: 44/48kHz, MCLK=64xfs
+	ret = snd_soc_write(codec, TAS5713_CLOCK_CTRL, 0x60);
+
+	// I2S 24bit
+	ret = snd_soc_write(codec, TAS5713_SERIAL_DATA_INTERFACE, 0x05);
+
+	// Unmute
+	ret = snd_soc_write(codec, TAS5713_SYSTEM_CTRL2, 0x00);
+	ret = snd_soc_write(codec, TAS5713_SOFT_MUTE, 0x00);
+
+	// Set volume to 0db
+	ret = snd_soc_write(codec, TAS5713_VOL_MASTER, 0x00);
+
+	// Now start programming the default initialization sequence
+	for (i = 0; i < ARRAY_SIZE(tas5713_init_sequence); ++i) {
+		ret = i2c_master_send(i2c,
+				     tas5713_init_sequence[i].data,
+				     tas5713_init_sequence[i].size);
+
+		if (ret < 0) {
+			printk(KERN_INFO "TAS5713 CODEC PROBE: InitSeq returns: %d\n", ret);
+		}
+	}
+
+	// Unmute
+	ret = snd_soc_write(codec, TAS5713_SYSTEM_CTRL2, 0x00);
+
+
+	return 0;
+}
+
+
+static struct snd_soc_codec_driver soc_codec_dev_tas5713 = {
+	.probe = tas5713_probe,
+	.remove = tas5713_remove,
+	.controls = tas5713_snd_controls,
+	.num_controls = ARRAY_SIZE(tas5713_snd_controls),
+};
+
+
+
+
+/*
+ *   ___ ___ ___   ___      _
+ *  |_ _|_  ) __| |   \ _ _(_)_ _____ _ _
+ *   | | / / (__  | |) | '_| \ V / -_) '_|
+ *  |___/___\___| |___/|_| |_|\_/\___|_|
+ *
+ */
+
+static const struct reg_default tas5713_reg_defaults[] = {
+	{ 0x07 ,0x80 },     // R7  - VOL_MASTER    - -40dB
+	{ 0x08 ,  30 },     // R8  - VOL_CH1	   -   0dB
+	{ 0x09 ,  30 },     // R9  - VOL_CH2       -   0dB
+	{ 0x0A ,0x80 },     // R10 - VOL_HEADPHONE - -40dB
+};
+
+
+static bool tas5713_reg_volatile(struct device *dev, unsigned int reg)
+{
+	switch (reg) {
+		case TAS5713_DEVICE_ID:
+		case TAS5713_ERROR_STATUS:
+			return true;
+	default:
+			return false;
+	}
+}
+
+
+static const struct of_device_id tas5713_of_match[] = {
+	{ .compatible = "ti,tas5713", },
+	{ }
+};
+MODULE_DEVICE_TABLE(of, tas5713_of_match);
+
+
+static struct regmap_config tas5713_regmap_config = {
+	.reg_bits = 8,
+	.val_bits = 8,
+
+	.max_register = TAS5713_MAX_REGISTER,
+	.volatile_reg = tas5713_reg_volatile,
+
+	.cache_type = REGCACHE_RBTREE,
+	.reg_defaults = tas5713_reg_defaults,
+	.num_reg_defaults = ARRAY_SIZE(tas5713_reg_defaults),
+};
+
+
+static int tas5713_i2c_probe(struct i2c_client *i2c,
+			    const struct i2c_device_id *id)
+{
+	int ret;
+
+	priv_data = devm_kzalloc(&i2c->dev, sizeof *priv_data, GFP_KERNEL);
+	if (!priv_data)
+		return -ENOMEM;
+
+	priv_data->regmap = devm_regmap_init_i2c(i2c, &tas5713_regmap_config);
+	if (IS_ERR(priv_data->regmap)) {
+		ret = PTR_ERR(priv_data->regmap);
+		return ret;
+	}
+
+	i2c_set_clientdata(i2c, priv_data);
+
+	ret = snd_soc_register_codec(&i2c->dev,
+				     &soc_codec_dev_tas5713, &tas5713_dai, 1);
+
+	return ret;
+}
+
+
+static int tas5713_i2c_remove(struct i2c_client *i2c)
+{
+	snd_soc_unregister_codec(&i2c->dev);
+	i2c_set_clientdata(i2c, NULL);
+
+	kfree(priv_data);
+
+	return 0;
+}
+
+
+static const struct i2c_device_id tas5713_i2c_id[] = {
+	{ "tas5713", 0 },
+	{ }
+};
+
+MODULE_DEVICE_TABLE(i2c, tas5713_i2c_id);
+
+
+static struct i2c_driver tas5713_i2c_driver = {
+	.driver = {
+		.name = "tas5713",
+		.owner = THIS_MODULE,
+		.of_match_table = tas5713_of_match,
+	},
+	.probe = tas5713_i2c_probe,
+	.remove = tas5713_i2c_remove,
+	.id_table = tas5713_i2c_id
+};
+
+
+static int __init tas5713_modinit(void)
+{
+	int ret = 0;
+
+	ret = i2c_add_driver(&tas5713_i2c_driver);
+	if (ret) {
+		printk(KERN_ERR "Failed to register tas5713 I2C driver: %d\n",
+		       ret);
+	}
+
+	return ret;
+}
+module_init(tas5713_modinit);
+
+
+static void __exit tas5713_exit(void)
+{
+	i2c_del_driver(&tas5713_i2c_driver);
+}
+module_exit(tas5713_exit);
+
+
+MODULE_AUTHOR("Sebastian Eickhoff <basti.eickhoff@googlemail.com>");
+MODULE_DESCRIPTION("ASoC driver for TAS5713");
+MODULE_LICENSE("GPL v2");
--- /dev/null
+++ b/sound/soc/codecs/tas5713.h
@@ -0,0 +1,210 @@
+/*
+ * ASoC Driver for TAS5713
+ *
+ * Author:      Sebastian Eickhoff <basti.eickhoff@googlemail.com>
+ *              Copyright 2014
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * version 2 as published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
+ * General Public License for more details.
+ */
+
+#ifndef _TAS5713_H
+#define _TAS5713_H
+
+
+// TAS5713 I2C-bus register addresses
+
+#define TAS5713_CLOCK_CTRL              0x00
+#define TAS5713_DEVICE_ID               0x01
+#define TAS5713_ERROR_STATUS            0x02
+#define TAS5713_SYSTEM_CTRL1            0x03
+#define TAS5713_SERIAL_DATA_INTERFACE   0x04
+#define TAS5713_SYSTEM_CTRL2            0x05
+#define TAS5713_SOFT_MUTE               0x06
+#define TAS5713_VOL_MASTER              0x07
+#define TAS5713_VOL_CH1                 0x08
+#define TAS5713_VOL_CH2                 0x09
+#define TAS5713_VOL_HEADPHONE           0x0A
+#define TAS5713_VOL_CONFIG              0x0E
+#define TAS5713_MODULATION_LIMIT        0x10
+#define TAS5713_IC_DLY_CH1              0x11
+#define TAS5713_IC_DLY_CH2              0x12
+#define TAS5713_IC_DLY_CH3              0x13
+#define TAS5713_IC_DLY_CH4              0x14
+
+#define TAS5713_START_STOP_PERIOD       0x1A
+#define TAS5713_OSC_TRIM                0x1B
+#define TAS5713_BKND_ERR                0x1C
+
+#define TAS5713_INPUT_MUX               0x20
+#define TAS5713_SRC_SELECT_CH4          0x21
+#define TAS5713_PWM_MUX                 0x25
+
+#define TAS5713_CH1_BQ0                 0x29
+#define TAS5713_CH1_BQ1                 0x2A
+#define TAS5713_CH1_BQ2                 0x2B
+#define TAS5713_CH1_BQ3                 0x2C
+#define TAS5713_CH1_BQ4                 0x2D
+#define TAS5713_CH1_BQ5                 0x2E
+#define TAS5713_CH1_BQ6                 0x2F
+#define TAS5713_CH1_BQ7                 0x58
+#define TAS5713_CH1_BQ8                 0x59
+
+#define TAS5713_CH2_BQ0                 0x30
+#define TAS5713_CH2_BQ1                 0x31
+#define TAS5713_CH2_BQ2                 0x32
+#define TAS5713_CH2_BQ3                 0x33
+#define TAS5713_CH2_BQ4                 0x34
+#define TAS5713_CH2_BQ5                 0x35
+#define TAS5713_CH2_BQ6                 0x36
+#define TAS5713_CH2_BQ7                 0x5C
+#define TAS5713_CH2_BQ8                 0x5D
+
+#define TAS5713_CH4_BQ0                 0x5A
+#define TAS5713_CH4_BQ1                 0x5B
+#define TAS5713_CH3_BQ0                 0x5E
+#define TAS5713_CH3_BQ1                 0x5F
+
+#define TAS5713_DRC1_SOFTENING_FILTER_ALPHA_OMEGA       0x3B
+#define TAS5713_DRC1_ATTACK_RELEASE_RATE                0x3C
+#define TAS5713_DRC2_SOFTENING_FILTER_ALPHA_OMEGA       0x3E
+#define TAS5713_DRC2_ATTACK_RELEASE_RATE                0x3F
+#define TAS5713_DRC1_ATTACK_RELEASE_THRES               0x40
+#define TAS5713_DRC2_ATTACK_RELEASE_THRES               0x43
+#define TAS5713_DRC_CTRL                                0x46
+
+#define TAS5713_BANK_SW_CTRL            0x50
+#define TAS5713_CH1_OUTPUT_MIXER        0x51
+#define TAS5713_CH2_OUTPUT_MIXER        0x52
+#define TAS5713_CH1_INPUT_MIXER         0x53
+#define TAS5713_CH2_INPUT_MIXER         0x54
+#define TAS5713_OUTPUT_POST_SCALE       0x56
+#define TAS5713_OUTPUT_PRESCALE         0x57
+
+#define TAS5713_IDF_POST_SCALE          0x62
+
+#define TAS5713_CH1_INLINE_MIXER        0x70
+#define TAS5713_CH1_INLINE_DRC_EN_MIXER 0x71
+#define TAS5713_CH1_R_CHANNEL_MIXER     0x72
+#define TAS5713_CH1_L_CHANNEL_MIXER     0x73
+#define TAS5713_CH2_INLINE_MIXER        0x74
+#define TAS5713_CH2_INLINE_DRC_EN_MIXER 0x75
+#define TAS5713_CH2_L_CHANNEL_MIXER     0x76
+#define TAS5713_CH2_R_CHANNEL_MIXER     0x77
+
+#define TAS5713_UPDATE_DEV_ADDR_KEY     0xF8
+#define TAS5713_UPDATE_DEV_ADDR_REG     0xF9
+
+#define TAS5713_REGISTER_COUNT          0x46
+#define TAS5713_MAX_REGISTER            0xF9
+
+
+// Bitmasks for registers
+#define TAS5713_SOFT_MUTE_ALL           0x07
+
+
+
+struct tas5713_init_command {
+        const int size;
+        const char *const data;
+};
+
+static const struct tas5713_init_command tas5713_init_sequence[] = {
+
+        // Trim oscillator
+    { .size = 2,  .data = "\x1B\x00" },
+    // System control register 1 (0x03): block DC
+    { .size = 2,  .data = "\x03\x80" },
+    // Mute everything
+    { .size = 2,  .data = "\x05\x40" },
+    // Modulation limit register (0x10): 97.7%
+    { .size = 2,  .data = "\x10\x02" },
+    // Interchannel delay registers
+    // (0x11, 0x12, 0x13, and 0x14): BD mode
+    { .size = 2,  .data = "\x11\xB8" },
+    { .size = 2,  .data = "\x12\x60" },
+    { .size = 2,  .data = "\x13\xA0" },
+    { .size = 2,  .data = "\x14\x48" },
+    // PWM shutdown group register (0x19): no shutdown
+    { .size = 2,  .data = "\x19\x00" },
+    // Input multiplexer register (0x20): BD mode
+    { .size = 2,  .data = "\x20\x00\x89\x77\x72" },
+    // PWM output mux register (0x25)
+    // Channel 1 --> OUTA, channel 1 neg --> OUTB
+    // Channel 2 --> OUTC, channel 2 neg --> OUTD
+    { .size = 5,  .data = "\x25\x01\x02\x13\x45" },
+    // DRC control (0x46): DRC off
+    { .size = 5,  .data = "\x46\x00\x00\x00\x00" },
+    // BKND_ERR register (0x1C): 299ms reset period
+    { .size = 2,  .data = "\x1C\x07" },
+    // Mute channel 3
+    { .size = 2,  .data = "\x0A\xFF" },
+    // Volume configuration register (0x0E): volume slew 512 steps
+    { .size = 2,  .data = "\x0E\x90" },
+    // Clock control register (0x00): 44/48kHz, MCLK=64xfs
+    { .size = 2,  .data = "\x00\x60" },
+    // Bank switch and eq control (0x50): no bank switching
+    { .size = 5,  .data = "\x50\x00\x00\x00\x00" },
+    // Volume registers (0x07, 0x08, 0x09, 0x0A)
+    { .size = 2,  .data = "\x07\x20" },
+    { .size = 2,  .data = "\x08\x30" },
+    { .size = 2,  .data = "\x09\x30" },
+    { .size = 2,  .data = "\x0A\xFF" },
+    // 0x72, 0x73, 0x76, 0x77 input mixer:
+    // no intermix between channels
+    { .size = 5,  .data = "\x72\x00\x00\x00\x00" },
+    { .size = 5,  .data = "\x73\x00\x80\x00\x00" },
+    { .size = 5,  .data = "\x76\x00\x00\x00\x00" },
+    { .size = 5,  .data = "\x77\x00\x80\x00\x00" },
+    // 0x70, 0x71, 0x74, 0x75 inline DRC mixer:
+    // no inline DRC inmix
+    { .size = 5,  .data = "\x70\x00\x80\x00\x00" },
+    { .size = 5,  .data = "\x71\x00\x00\x00\x00" },
+    { .size = 5,  .data = "\x74\x00\x80\x00\x00" },
+    { .size = 5,  .data = "\x75\x00\x00\x00\x00" },
+    // 0x56, 0x57 Output scale
+    { .size = 5,  .data = "\x56\x00\x80\x00\x00" },
+    { .size = 5,  .data = "\x57\x00\x02\x00\x00" },
+    // 0x3B, 0x3c
+    { .size = 9,  .data = "\x3B\x00\x08\x00\x00\x00\x78\x00\x00" },
+    { .size = 9,  .data = "\x3C\x00\x00\x01\x00\xFF\xFF\xFF\x00" },
+    { .size = 9,  .data = "\x3E\x00\x08\x00\x00\x00\x78\x00\x00" },
+    { .size = 9,  .data = "\x3F\x00\x00\x01\x00\xFF\xFF\xFF\x00" },
+    { .size = 9,  .data = "\x40\x00\x00\x01\x00\xFF\xFF\xFF\x00" },
+    { .size = 9,  .data = "\x43\x00\x00\x01\x00\xFF\xFF\xFF\x00" },
+    // 0x51, 0x52: output mixer
+    { .size = 9,  .data = "\x51\x00\x80\x00\x00\x00\x00\x00\x00" },
+    { .size = 9,  .data = "\x52\x00\x80\x00\x00\x00\x00\x00\x00" },
+    // PEQ defaults
+    { .size = 21,  .data = "\x29\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x2A\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x2B\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x2C\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x2D\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x2E\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x2F\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x30\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x31\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x32\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x33\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x34\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x35\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x36\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x58\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x59\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x5C\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x5D\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x5E\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x5F\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x5A\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+    { .size = 21,  .data = "\x5B\x00\x80\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00" },
+};
+
+
+#endif  /* _TAS5713_H */
