From 6c2d32478159fffff0b85abb6817a21bb2338231 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Sun, 24 Mar 2013 19:26:27 +0100
Subject: [PATCH] rt2x00: rt2800soc: fix rt2800soc_disable_radio for RT3883

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/rt2x00/rt2800soc.c |    9 ++++++++-
 1 file changed, 8 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/rt2x00/rt2800soc.c
+++ b/drivers/net/wireless/rt2x00/rt2800soc.c
@@ -51,9 +51,16 @@ static bool rt2800soc_hwcrypt_disabled(s
 
 static void rt2800soc_disable_radio(struct rt2x00_dev *rt2x00dev)
 {
+	u32 reg;
+
 	rt2800_disable_radio(rt2x00dev);
 	rt2x00mmio_register_write(rt2x00dev, PWR_PIN_CFG, 0);
-	rt2x00mmio_register_write(rt2x00dev, TX_PIN_CFG, 0);
+
+	reg = 0;
+	if (rt2x00_rt(rt2x00dev, RT3883))
+		rt2x00_set_field32(&reg, TX_PIN_CFG_RFTR_EN, 1);
+
+	rt2x00mmio_register_write(rt2x00dev, TX_PIN_CFG, reg);
 }
 
 static int rt2800soc_set_device_state(struct rt2x00_dev *rt2x00dev,
