From ce24753015125e11d87764dca9740fde33ccd455 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 4 Feb 2015 10:02:24 +0000
Subject: [PATCH 102/114] pinctrl-bcm2835: bcm2835_gpio_direction_output must
 set the value

---
 drivers/pinctrl/pinctrl-bcm2835.c | 9 ++++++++-
 1 file changed, 8 insertions(+), 1 deletion(-)

--- a/drivers/pinctrl/pinctrl-bcm2835.c
+++ b/drivers/pinctrl/pinctrl-bcm2835.c
@@ -355,7 +355,14 @@ static int bcm2835_gpio_get(struct gpio_
 static int bcm2835_gpio_direction_output(struct gpio_chip *chip,
 		unsigned offset, int value)
 {
-	return pinctrl_gpio_direction_output(chip->base + offset);
+	struct bcm2835_pinctrl *pc = dev_get_drvdata(chip->dev);
+	int ret;
+
+	ret = pinctrl_gpio_direction_output(chip->base + offset);
+	if (ret >= 0)
+		bcm2835_gpio_set_bit(pc, value ? GPSET0 : GPCLR0, offset);
+
+	return ret;
 }
 
 static void bcm2835_gpio_set(struct gpio_chip *chip, unsigned offset, int value)
