From: Hante Meuleman <meuleman@broadcom.com>
Date: Wed, 18 Mar 2015 13:25:23 +0100
Subject: [PATCH] brcmfmac: Update msgbuf commonring size for improved
 throughput.

Reviewed-by: Arend Van Spriel <arend@broadcom.com>
Reviewed-by: Pieter-Paul Giesberts <pieterpg@broadcom.com>
Signed-off-by: Hante Meuleman <meuleman@broadcom.com>
Signed-off-by: Arend van Spriel <arend@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---

--- a/drivers/net/wireless/brcm80211/brcmfmac/msgbuf.h
+++ b/drivers/net/wireless/brcm80211/brcmfmac/msgbuf.h
@@ -17,11 +17,11 @@
 
 #ifdef CPTCFG_BRCMFMAC_PROTO_MSGBUF
 
-#define BRCMF_H2D_MSGRING_CONTROL_SUBMIT_MAX_ITEM	20
-#define BRCMF_H2D_MSGRING_RXPOST_SUBMIT_MAX_ITEM	256
-#define BRCMF_D2H_MSGRING_CONTROL_COMPLETE_MAX_ITEM	20
+#define BRCMF_H2D_MSGRING_CONTROL_SUBMIT_MAX_ITEM	64
+#define BRCMF_H2D_MSGRING_RXPOST_SUBMIT_MAX_ITEM	512
+#define BRCMF_D2H_MSGRING_CONTROL_COMPLETE_MAX_ITEM	64
 #define BRCMF_D2H_MSGRING_TX_COMPLETE_MAX_ITEM		1024
-#define BRCMF_D2H_MSGRING_RX_COMPLETE_MAX_ITEM		256
+#define BRCMF_D2H_MSGRING_RX_COMPLETE_MAX_ITEM		512
 #define BRCMF_H2D_TXFLOWRING_MAX_ITEM			512
 
 #define BRCMF_H2D_MSGRING_CONTROL_SUBMIT_ITEMSIZE	40
