--- a/hostapd/Makefile
+++ b/hostapd/Makefile
@@ -168,6 +168,9 @@ endif
 ifdef CONFIG_NO_CTRL_IFACE
 CFLAGS += -DCONFIG_NO_CTRL_IFACE
 else
+ifdef CONFIG_CTRL_IFACE_MIB
+CFLAGS += -DCONFIG_CTRL_IFACE_MIB
+endif
 OBJS += ctrl_iface.o
 OBJS += ../src/ap/ctrl_iface_ap.o
 endif
--- a/hostapd/ctrl_iface.c
+++ b/hostapd/ctrl_iface.c
@@ -1953,6 +1953,7 @@ static void hostapd_ctrl_iface_receive(i
 						      reply_size);
 	} else if (os_strcmp(buf, "STATUS-DRIVER") == 0) {
 		reply_len = hostapd_drv_status(hapd, reply, reply_size);
+#ifdef CONFIG_CTRL_IFACE_MIB
 	} else if (os_strcmp(buf, "MIB") == 0) {
 		reply_len = ieee802_11_get_mib(hapd, reply, reply_size);
 		if (reply_len >= 0) {
@@ -1994,6 +1995,7 @@ static void hostapd_ctrl_iface_receive(i
 	} else if (os_strncmp(buf, "STA-NEXT ", 9) == 0) {
 		reply_len = hostapd_ctrl_iface_sta_next(hapd, buf + 9, reply,
 							reply_size);
+#endif
 	} else if (os_strcmp(buf, "ATTACH") == 0) {
 		if (hostapd_ctrl_iface_attach(hapd, &from, fromlen))
 			reply_len = -1;
--- a/wpa_supplicant/Makefile
+++ b/wpa_supplicant/Makefile
@@ -837,6 +837,9 @@ ifdef CONFIG_WNM
 OBJS += ../src/ap/wnm_ap.o
 endif
 ifdef CONFIG_CTRL_IFACE
+ifdef CONFIG_CTRL_IFACE_MIB
+CFLAGS += -DCONFIG_CTRL_IFACE_MIB
+endif
 OBJS += ../src/ap/ctrl_iface_ap.o
 endif
 
--- a/wpa_supplicant/ctrl_iface.c
+++ b/wpa_supplicant/ctrl_iface.c
@@ -1795,7 +1795,7 @@ static int wpa_supplicant_ctrl_iface_sta
 			pos += ret;
 		}
 
-#ifdef CONFIG_AP
+#if defined(CONFIG_AP) && defined(CONFIG_CTRL_IFACE_MIB)
 		if (wpa_s->ap_iface) {
 			pos += ap_ctrl_iface_wpa_get_status(wpa_s, pos,
 							    end - pos,
@@ -7896,6 +7896,7 @@ char * wpa_supplicant_ctrl_iface_process
 			reply_len = -1;
 	} else if (os_strncmp(buf, "NOTE ", 5) == 0) {
 		wpa_printf(MSG_INFO, "NOTE: %s", buf + 5);
+#ifdef CONFIG_CTRL_IFACE_MIB
 	} else if (os_strcmp(buf, "MIB") == 0) {
 		reply_len = wpa_sm_get_mib(wpa_s->wpa, reply, reply_size);
 		if (reply_len >= 0) {
@@ -7903,6 +7904,7 @@ char * wpa_supplicant_ctrl_iface_process
 						      reply + reply_len,
 						      reply_size - reply_len);
 		}
+#endif
 	} else if (os_strncmp(buf, "STATUS", 6) == 0) {
 		reply_len = wpa_supplicant_ctrl_iface_status(
 			wpa_s, buf + 6, reply, reply_size);
@@ -8353,6 +8355,7 @@ char * wpa_supplicant_ctrl_iface_process
 		reply_len = wpa_supplicant_ctrl_iface_bss(
 			wpa_s, buf + 4, reply, reply_size);
 #ifdef CONFIG_AP
+#ifdef CONFIG_CTRL_IFACE_MIB
 	} else if (os_strcmp(buf, "STA-FIRST") == 0) {
 		reply_len = ap_ctrl_iface_sta_first(wpa_s, reply, reply_size);
 	} else if (os_strncmp(buf, "STA ", 4) == 0) {
@@ -8361,12 +8364,15 @@ char * wpa_supplicant_ctrl_iface_process
 	} else if (os_strncmp(buf, "STA-NEXT ", 9) == 0) {
 		reply_len = ap_ctrl_iface_sta_next(wpa_s, buf + 9, reply,
 						   reply_size);
+#endif
+#ifdef CONFIG_CTRL_IFACE_MIB
 	} else if (os_strncmp(buf, "DEAUTHENTICATE ", 15) == 0) {
 		if (ap_ctrl_iface_sta_deauthenticate(wpa_s, buf + 15))
 			reply_len = -1;
 	} else if (os_strncmp(buf, "DISASSOCIATE ", 13) == 0) {
 		if (ap_ctrl_iface_sta_disassociate(wpa_s, buf + 13))
 			reply_len = -1;
+#endif
 	} else if (os_strncmp(buf, "CHAN_SWITCH ", 12) == 0) {
 		if (ap_ctrl_iface_chanswitch(wpa_s, buf + 12))
 			reply_len = -1;
--- a/src/ap/ctrl_iface_ap.c
+++ b/src/ap/ctrl_iface_ap.c
@@ -22,6 +22,7 @@
 #include "ctrl_iface_ap.h"
 #include "ap_drv_ops.h"
 
+#ifdef CONFIG_CTRL_IFACE_MIB
 
 static int hostapd_get_sta_tx_rx(struct hostapd_data *hapd,
 				 struct sta_info *sta,
@@ -224,6 +225,7 @@ int hostapd_ctrl_iface_sta_next(struct h
 	return hostapd_ctrl_iface_sta_mib(hapd, sta->next, buf, buflen);
 }
 
+#endif
 
 #ifdef CONFIG_P2P_MANAGER
 static int p2p_manager_disconnect(struct hostapd_data *hapd, u16 stype,
--- a/src/ap/ieee802_1x.c
+++ b/src/ap/ieee802_1x.c
@@ -2337,6 +2337,7 @@ static const char * bool_txt(Boolean boo
 	return bool_val ? "TRUE" : "FALSE";
 }
 
+#ifdef CONFIG_CTRL_IFACE_MIB
 
 int ieee802_1x_get_mib(struct hostapd_data *hapd, char *buf, size_t buflen)
 {
@@ -2512,6 +2513,7 @@ int ieee802_1x_get_mib_sta(struct hostap
 	return len;
 }
 
+#endif
 
 static void ieee802_1x_finished(struct hostapd_data *hapd,
 				struct sta_info *sta, int success,
--- a/src/ap/wpa_auth.c
+++ b/src/ap/wpa_auth.c
@@ -2999,6 +2999,7 @@ static const char * wpa_bool_txt(int boo
 	return bool ? "TRUE" : "FALSE";
 }
 
+#ifdef CONFIG_CTRL_IFACE_MIB
 
 #define RSN_SUITE "%02x-%02x-%02x-%d"
 #define RSN_SUITE_ARG(s) \
@@ -3143,7 +3144,7 @@ int wpa_get_mib_sta(struct wpa_state_mac
 
 	return len;
 }
-
+#endif
 
 void wpa_auth_countermeasures_start(struct wpa_authenticator *wpa_auth)
 {
--- a/src/rsn_supp/wpa.c
+++ b/src/rsn_supp/wpa.c
@@ -2032,6 +2032,8 @@ static u32 wpa_key_mgmt_suite(struct wpa
 }
 
 
+#ifdef CONFIG_CTRL_IFACE_MIB
+
 #define RSN_SUITE "%02x-%02x-%02x-%d"
 #define RSN_SUITE_ARG(s) \
 ((s) >> 24) & 0xff, ((s) >> 16) & 0xff, ((s) >> 8) & 0xff, (s) & 0xff
@@ -2115,6 +2117,7 @@ int wpa_sm_get_mib(struct wpa_sm *sm, ch
 
 	return (int) len;
 }
+#endif
 #endif /* CONFIG_CTRL_IFACE */
 
 
--- a/wpa_supplicant/ap.c
+++ b/wpa_supplicant/ap.c
@@ -1015,7 +1015,7 @@ int wpas_ap_wps_nfc_report_handover(stru
 #endif /* CONFIG_WPS */
 
 
-#ifdef CONFIG_CTRL_IFACE
+#if defined(CONFIG_CTRL_IFACE) && defined(CONFIG_CTRL_IFACE_MIB)
 
 int ap_ctrl_iface_sta_first(struct wpa_supplicant *wpa_s,
 			    char *buf, size_t buflen)
