From 7875b470c9d80dff2d58ae9692adb3a2b5814a89 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Fri, 20 Feb 2015 11:22:05 +0100
Subject: [PATCH] ARM: BCM5301X: Fix default state of power LEDs on Netgear
 R6250
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

We want green LED to be enabled by default.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm4708-netgear-r6250.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
@@ -45,13 +45,13 @@
 		power0 {
 			label = "bcm53xx:green:power";
 			gpios = <&chipcommon 2 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
+			linux,default-trigger = "default-on";
 		};
 
 		power1 {
 			label = "bcm53xx:amber:power";
 			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-on";
+			linux,default-trigger = "default-off";
 		};
 
 		usb {
