From 0d7388de0911c1a4fc4a8a3898ef9d0ab818ca08 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Tue, 7 Apr 2015 18:35:15 +0200
Subject: [PATCH] mtd: spi-nor: add support for the Macronix MX25L512E SPI
 flash chip

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/mtd/spi-nor/spi-nor.c |    1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -517,6 +517,7 @@ static const struct spi_device_id spi_no
 	{ "640s33b",  INFO(0x898913, 0, 64 * 1024, 128, 0) },
 
 	/* Macronix */
+	{ "mx25l512e",   INFO(0xc22010, 0, 64 * 1024,   1, SECT_4K) },
 	{ "mx25l2005a",  INFO(0xc22012, 0, 64 * 1024,   4, SECT_4K) },
 	{ "mx25l4005a",  INFO(0xc22013, 0, 64 * 1024,   8, SECT_4K) },
 	{ "mx25l8005",   INFO(0xc22014, 0, 64 * 1024,  16, 0) },
