/dts-v1/;

/include/ "bcm6358.dtsi"

/ {
	model = "SFR Neuf Box 4 (Foxconn)";
	compatible = "sfr,nb4-fxc-r1", "brcm,bcm6358";

	spi-gpio {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "spi-gpio";

		gpio-mosi = <&gpio0 7 0>;
		gpio-sck = <&gpio0 6 0>;
		num-chipselects = <0>;

		hc595: gpio-spi-controller@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			registers-number = <1>;
			spi-max-frequency = <100000>;

			gpio-controller;
			#gpio-cells = <2>;
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;
		debounce-interval = <60>;

		service {
			label = "service";
			gpios = <&gpio0 27 1>;
			linux,code = <0x100>;
		};
		clip {
			label = "clip";
			gpios = <&gpio0 31 1>;
			linux,code = <0x101>;
		};
		reset {
			label = "reset";
			gpios = <&gpio1 2 1>;
			linux,code = <0x198>;
		};
		wps {
			label = "wps";
			gpios = <&gpio1 5 1>;
			linux,code = <0x211>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		traffic_white {
			label = "NB4-FXC-r1:white:traffic";
			gpios = <&gpio0 2 0>;
		};
		service_blue {
			label = "NB4-FXC-r1:blue:service";
			gpios = <&gpio0 4 0>;
		};
		wifi_white {
			label = "NB4-FXC-r1:white:wifi";
			gpios = <&gpio0 15 0>;
		};
		service_red {
			label = "NB4-FXC-r1:red:service";
			gpios = <&gpio0 29 0>;
		};
		service_green {
			label = "NB4-FXC-r1:green:service";
			gpios = <&gpio0 30 0>;
		};
		alarm_white {
			label = "NB4-FXC-r1:white:alarm";
			gpios = <&hc595 0 1>;
		};
		tv_white {
			label = "NB4-FXC-r1:white:tv";
			gpios = <&hc595 2 1>;
		};
		tel_white {
			label = "NB4-FXC-r1:white:tel";
			gpios = <&hc595 3 1>;
		};
		adsl_white {
			label = "NB4-FXC-r0:white:adsl";
			gpios = <&hc595 4 1>;
		};
	};
};
