From a2a3c09223aa520e08cc34c496dc286843eecf92 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 26 Jan 2015 15:26:10 +0000
Subject: [PATCH 082/114] BCM2708_DT: Correct length of the peripheral space

---
 arch/arm/boot/dts/bcm2708.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/bcm2708.dtsi
+++ b/arch/arm/boot/dts/bcm2708.dtsi
@@ -15,7 +15,7 @@
 		compatible = "simple-bus";
 		#address-cells = <1>;
 		#size-cells = <1>;
-		ranges = <0x7e000000 0x20000000 0x02000000>;
+		ranges = <0x7e000000 0x20000000 0x01000000>;
 
 		intc: interrupt-controller {
 			compatible = "brcm,bcm2708-armctrl-ic";
