#!/bin/sh
#
# Copyright (C) 2011 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/ar71xx.sh

board=$(ar71xx_board_name)

case "$board" in
airgateway)
	ucidef_set_led_wlan "wlan" "WLAN" "ubnt:blue:wlan" "phy0tpt"
	;;
alfa-nx)
	ucidef_set_led_netdev "wan" "WAN" "alfa:green:led_2" "eth0"
	ucidef_set_led_netdev "lan" "LAN" "alfa:green:led_3" "eth1"
	;;

all0258n)
	ucidef_set_rssimon "wlan0" "40000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "all0258n:red:rssilow" "wlan0" "1" "40" "0" "6"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "all0258n:yellow:rssimedium" "wlan0" "30" "80" "-29" "5"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "all0258n:green:rssihigh" "wlan0" "70" "100" "-69" "8"
	;;

all0315n)
	ucidef_set_rssimon "wlan0" "40000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "all0315n:red:rssilow" "wlan0" "1" "40" "0" "6"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "all0315n:yellow:rssimedium" "wlan0" "30" "80" "-29" "5"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "all0315n:green:rssihigh" "wlan0" "70" "100" "-69" "8"
	;;

antminer-s1)
	ucidef_set_led_default "sys" "SYS" "bitmain:green:sys" "0"
	ucidef_set_led_wlan "wlan" "WLAN" "bitmain:green:wlan" "phy0tpt"
	;;

antminer-s3)
	ucidef_set_led_wlan "wlan" "WLAN" "bitmain:green:wlan" "phy0tpt"
	ucidef_set_led_default "sys" "SYS" "bitmain:green:sys" "0"
	ucidef_set_led_default "lan" "LAN" "bitmain:yellow:lan" "0"
	;;

ap113)
	ucidef_set_led_usbdev "usb" "USB" "ap113:green:usb" "1-1"
	;;

bsb)
	ucidef_set_led_default "sys" "SYS" "bsb:red:sys" "1"
	;;

bullet-m | \
nanostation-m | \
rocket-m | \
rocket-m-xw | \
nanostation-m-xw | \
loco-m-xw)
	ucidef_set_led_rssi "rssilow" "RSSILOW" "ubnt:red:link1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "ubnt:orange:link2" "wlan0" "26" "100" "-25" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "ubnt:green:link3" "wlan0" "51" "100" "-50" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "ubnt:green:link4" "wlan0" "76" "100" "-75" "13"
	;;

bxu2000n-2-a1)
	ucidef_set_led_wlan "wlan" "WLAN" "bhu:green:wlan" "phy0tpt"
	;;

cap4200ag)
	ucidef_set_led_default "lan_green" "LAN_GREEN" "senao:green:lan" "1"
	ucidef_set_led_wlan "wlan_amber" "WLAN_AMBER" "senao:amber:wlan" "phy0tpt"
	ucidef_set_led_wlan "wlan_green" "WLAN_GREEN" "senao:green:wlan" "phy1tpt"
	;;

carambola2)
	ucidef_set_led_netdev "lan" "LAN" "carambola2:orange:eth0" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "carambola2:orange:eth1" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "carambola2:green:wlan" "phy0tpt"
	;;

cpe510)
	ucidef_set_led_switch "lan0" "LAN0" "tp-link:green:lan0" "switch0" "0x20"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x10"
	ucidef_set_rssimon "wlan0" "40000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:green:link1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:green:link2" "wlan0" "26" "100" "-25" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:green:link3" "wlan0" "51" "100" "-50" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:green:link4" "wlan0" "76" "100" "-75" "13"
	;;

db120)
	ucidef_set_led_usbdev "usb" "USB" "db120:green:usb" "1-1"
	;;

dragino2)
	ucidef_set_led_wlan "wlan" "WLAN" "dragino2:red:wlan" "phy0tpt"
	ucidef_set_led_netdev "lan" "LAN" "dragino2:red:lan" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "dragino2:red:wan" "eth1"
	;;

eap300v2)
	ucidef_set_led_netdev "lan" "LAN" "engenius:blue:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "engenius:blue:wlan" "phy0tpt"
	;;

f9k1115v2)
	ucidef_set_led_usbdev "usb2" "USB2" "belkin:green:usb2" "1-1"
	;;

rb-750)
	ucidef_set_led_default "act" "act" "rb750:green:act" "1"
	ucidef_set_led_netdev "port1" "port1" "rb750:green:port1" "eth1"
	ucidef_set_led_switch "port2" "port2" "rb750:green:port2" "switch0" "0x10"
	ucidef_set_led_switch "port3" "port3" "rb750:green:port3" "switch0" "0x08"
	ucidef_set_led_switch "port4" "port4" "rb750:green:port4" "switch0" "0x04"
	ucidef_set_led_switch "port5" "port5" "rb750:green:port5" "switch0" "0x02"
	;;

rb-2011l|\
rb-2011uas|\
rb-2011uias|\
rb-2011uas-2hnd|\
rb-2011uias-2hnd)
	ucidef_set_led_switch "eth6" "ETH6" "rb:green:eth6" "switch1" "0x20"
	ucidef_set_led_switch "eth7" "ETH7" "rb:green:eth7" "switch1" "0x10"
	ucidef_set_led_switch "eth8" "ETH8" "rb:green:eth8" "switch1" "0x08"
	ucidef_set_led_switch "eth9" "ETH9" "rb:green:eth9" "switch1" "0x04"
	ucidef_set_led_switch "eth10" "ETH10" "rb:green:eth10" "switch1" "0x02"
	;;

dhp-1565-a1)
	ucidef_set_led_switch "wan" "WAN" "d-link:green:planet" "switch0" "0x20"
	;;

dir-505-a1)
	ucidef_set_led_netdev "lan" "LAN" "d-link:green:power" "eth1"
	;;

dir-600-a1|\
dir-615-e1|\
dir-615-e4)
	ucidef_set_led_netdev "wan" "WAN" "d-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "d-link:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "d-link:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "d-link:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "d-link:green:lan4" "switch0" "0x10"
	;;

dir-615-c1)
	ucidef_set_led_netdev "wan" "WAN" "d-link:green:wan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "d-link:green:wlan" "phy0tpt"
	;;

dir-825-b1)
	ucidef_set_led_usbdev "usb" "USB" "d-link:blue:usb" "1-1"
	;;

dir-825-c1)
	ucidef_set_led_usbdev "usb" "USB" "d-link:blue:usb" "1-1"
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "d-link:blue:wlan2g" "phy0tpt"
	;;

dlan-pro-500-wp)
	ucidef_set_led_default "power" "System Power" "devolo:green:status" "1"
	ucidef_set_led_netdev "lan" "Ethernet Activity" "devolo:green:eth" "br-lan"
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "devolo:green:wlan-2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN 5 GHz" "devolo:blue:wlan-5g" "none"
	;;

dlan-pro-1200-ac)
	ucidef_set_led_wlan "wlan" "WLAN" "devolo:status:wlan" "phy0radio"
	ucidef_set_led_trigger_gpio "plcw" "dLAN" "devolo:status:dlan" "17" "0"
	ucidef_set_led_trigger_gpio "plcr" "dLAN" "devolo:error:dlan" "16" "0"
	;;

gl-inet)
	ucidef_set_led_netdev "lan" "LAN" "gl-connect:green:lan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "gl-connect:red:wlan" "phy0tpt"
	;;

esr900)
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "engenius:blue:wlan-2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN 5 GHz" "engenius:blue:wlan-5g" "phy1tpt"
	;;

esr1750)
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "esr1750:blue:wlan-2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN 5 GHz" "esr1750:blue:wlan-5g" "phy1tpt"
	;;

epg5000)
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "epg5000:blue:wlan-2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN 5 GHz" "epg5000:blue:wlan-5g" "phy0tpt"
	;;

hiwifi-hc6361)
	ucidef_set_led_netdev "inet" "INET" "hiwifi:blue:internet" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "hiwifi:blue:wlan-2p4" "phy0tpt"
	;;

hornet-ub | \
hornet-ub-x2)
	ucidef_set_led_netdev "lan" "LAN" "alfa:blue:lan" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "alfa:blue:wan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "alfa:blue:wlan" "phy0tpt"
	ucidef_set_led_usbdev "usb" "USB" "alfa:blue:usb" "1-1"
	;;

mc-mac1200r)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "mercury:green:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "mercury:green:wlan5g" "phy0tpt"
	;;

mr12)
	ucidef_set_led_netdev "wan" "WAN" "mr12:green:wan" "eth0"
	ucidef_set_led_wlan "wlan1" "WLAN1" "mr12:green:wifi1" "phy0assoc"
	ucidef_set_led_wlan "wlan2" "WLAN2" "mr12:green:wifi2" "phy0assoc"
	ucidef_set_led_wlan "wlan3" "WLAN3" "mr12:green:wifi3" "phy0assoc"
	ucidef_set_led_wlan "wlan4" "WLAN4" "mr12:green:wifi4" "phy0tpt"
	;;

mr16)
	ucidef_set_led_netdev "wan" "WAN" "mr16:green:wan" "eth0"
	ucidef_set_led_wlan "wlan1" "WLAN1" "mr16:green:wifi1" "phy0assoc"
	ucidef_set_led_wlan "wlan2" "WLAN2" "mr16:green:wifi2" "phy0assoc"
	ucidef_set_led_wlan "wlan3" "WLAN3" "mr16:green:wifi3" "phy0assoc"
	ucidef_set_led_wlan "wlan4" "WLAN4" "mr16:green:wifi4" "phy0tpt"
	;;

mr600)
	ucidef_set_led_wlan "wlan58" "WLAN58" "mr600:green:wlan58" "phy0tpt"
	;;

mr900 | \
mr900v2)
	ucidef_set_led_netdev "lan" "LAN" "mr900:blue:wan" "eth0"
	ucidef_set_led_wlan "wlan24" "WLAN24" "mr900:blue:wlan24" "phy0tpt"
	ucidef_set_led_wlan "wlan58" "WLAN58" "mr900:blue:wlan58" "phy1tpt"
	;;

mynet-n600)
	ucidef_set_led_netdev "wan" "WAN" "wd:blue:internet" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "wd:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "wd:green:lan2" "switch0" "0x10"
	ucidef_set_led_switch "lan3" "LAN3" "wd:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "wd:green:lan4" "switch0" "0x04"
	;;

mynet-rext)
	ucidef_set_led_netdev "lan" "LAN" "wd:blue:ethernet" "eth0"
	ucidef_set_rssimon "wlan0" "40000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "wd:blue:quality1" "wlan0" "1" "40" "0" "6"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "wd:blue:quality2" "wlan0" "30" "80" "-29" "5"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "wd:blue:quality3" "wlan0" "70" "100" "-69" "8"
	ucidef_set_led_wlan "wlan" "WLAN" "wd:blue:wireless" "phy0tpt"
	;;

mzk-w04u)
	ucidef_set_led_usbdev "usb" "USB" "planex:green:usb" "1-1"
	;;

mzk-w300nh)
	ucidef_set_led_wlan "wlan" "WLAN" "planex:green:wlan" "phy0tpt"
	;;

nbg460n_550n_550nh)
	ucidef_set_led_wlan "wlan" "WLAN" "nbg460n:green:wlan" "phy0tpt"
	;;

nbg6716)
	ucidef_set_led_netdev "wan" "WAN" "zyxel:white:internet" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "zyxel:white:wifi2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5" "WLAN5" "zyxel:white:wifi5g" "phy0tpt"
	ucidef_set_led_usbdev "usb1" "USB1" "zyxel:white:usb1" "2-1"
	ucidef_set_led_usbdev "usb2" "USB2" "zyxel:white:usb2" "1-1"
	;;

om2p | \
om2pv2 | \
om2p-hs | \
om2p-hsv2 | \
om2p-lc)
	ucidef_set_led_netdev "port1" "port1" "om2p:blue:wan" "eth0"
	ucidef_set_led_netdev "port2" "port2" "om2p:blue:lan" "eth1"
	;;

om5p | \
om5p-an)
	ucidef_set_led_netdev "port1" "port1" "om5p:blue:wan" "eth0"
	ucidef_set_led_netdev "port2" "port2" "om5p:blue:lan" "eth1"
	;;

qihoo-c301)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "qihoo:red:status" "phy1tpt"
	;;

smart-300)
	ucidef_set_led_netdev "wan" "WAN" "nc-link:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "nc-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "nc-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "nc-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "nc-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "nc-link:green:wlan" "phy0tpt"
	;;

tew-712br)
	ucidef_set_led_netdev "wan" "WAN" "trendnet:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "trendnet:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "trendnet:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "trendnet:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "trendnet:green:lan4" "switch0" "0x10"
	ucidef_set_led_wlan "wlan" "WLAN" "trendnet:green:wlan" "phy0tpt"
	;;

tew-732br)
	ucidef_set_led_netdev "wan" "WAN" "trendnet:green:wan" "eth1"
	;;

tl-mr11u | \
tl-mr3020 | \
tl-mr3040 | \
tl-mr3040-v2)
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan"  "eth0"
	;;

tl-mr3220 | \
tl-mr3420 )
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
	;;

tl-mr3220-v2)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
	;;

tl-mr3420-v2)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
	;;

tl-wa7210n-v2)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	ucidef_set_rssimon "wlan0" "40000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:green:signal1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:green:signal2" "wlan0" "26" "100" "-25" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:green:signal3" "wlan0" "51" "100" "-50" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:green:signal4" "wlan0" "76" "100" "-75" "13"
	;;

tl-wa750re)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:orange:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:orange:wlan" "phy0tpt"
	ucidef_set_rssimon "wlan0" "40000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:orange:signal1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:orange:signal2" "wlan0" "20" "100" "-19" "13"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "tp-link:orange:signal3" "wlan0" "40" "100" "-39" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:orange:signal4" "wlan0" "60" "100" "-59" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:orange:signal5" "wlan0" "80" "100" "-79" "13"
	;;

tl-wa850re)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:blue:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:blue:wlan" "phy0tpt"
	ucidef_set_rssimon "wlan0" "40000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:blue:signal1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:blue:signal2" "wlan0" "20" "100" "-19" "13"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "tp-link:blue:signal3" "wlan0" "40" "100" "-39" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:blue:signal4" "wlan0" "60" "100" "-59" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:blue:signal5" "wlan0" "80" "100" "-79" "13"
	;;

tl-wa701nd-v2)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wa860re)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wa901nd)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	;;

tl-wa901nd-v2)
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wdr3500)
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:usb" "1-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "tp-link:green:wlan2g" "phy0tpt"
	;;

tl-wdr4300)
	ucidef_set_led_usbdev "usb1" "USB1" "tp-link:green:usb1" "1-1.1"
	ucidef_set_led_usbdev "usb2" "USB2" "tp-link:green:usb2" "1-1.2"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "tp-link:blue:wlan2g" "phy0tpt"
	;;

tl-wdr4900-v2)
	ucidef_set_led_usbdev "usb1" "USB1" "tp-link:green:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "tp-link:green:usb2" "2-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "tp-link:blue:wlan2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "tp-link:blue:wlan5g" "phy1tpt"
	;;

archer-c5|\
archer-c7)
	ucidef_set_led_usbdev "usb1" "USB1" "tp-link:green:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "tp-link:green:usb2" "2-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "tp-link:blue:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "tp-link:blue:wlan5g" "phy0tpt"
	;;

tl-wr741nd)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x10"
	;;

tl-wr741nd-v4)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wr841n-v8 | \
tl-wr941nd-v5)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wa830re-v2)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wr841n-v9)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wr842n-v2)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
	;;

tl-wa801nd-v2 | \
tl-wa901nd-v3)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wr941nd | \
tl-wr1041n-v2)
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wr1043nd | \
tl-wr1043nd-v2)
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:usb" "1-1"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;

tl-wr2543n)
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:usb" "1-1"
	;;

tube2h)
	ucidef_set_led_netdev "lan" "LAN" "alfa:blue:lan" "eth0"
	ucidef_set_rssimon "wlan0" "40000" "1"
	ucidef_set_led_rssi "signal1" "SIGNAL1" "alfa:red:signal1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "signal2" "SIGNAL2" "alfa:orange:signal2" "wlan0" "26" "100" "-25" "13"
	ucidef_set_led_rssi "signal3" "SIGNAL3" "alfa:green:signal3" "wlan0" "51" "100" "-50" "13"
	ucidef_set_led_rssi "signal4" "SIGNAL4" "alfa:green:signal4" "wlan0" "76" "100" "-75" "13"
	;;

wrt160nl)
	ucidef_set_led_wlan "wlan" "WLAN" "wrt160nl:blue:wlan" "phy0tpt"
	;;

wndap360)
        ucidef_set_led_power "power" "POWER GREEN" "netgear:green:power" "1"
        ;;

wndr3700)
	ucidef_set_led_default "wan" "WAN LED (green)" "netgear:green:wan" "0"
	ucidef_set_led_usbdev "usb" "USB" "netgear:green:usb" "1-1"
	;;

r6100)
	ucidef_set_led_netdev "wan" "WAN (green)" "netgear:green:wan" "eth0"
	ucidef_set_led_usbdev "usb" "USB" "netgear:blue:usb" "1-1"
	ucidef_set_led_wlan "wlan" "WLAN" "netgear:blue:wlan" "phy1tpt"
	;;

wndr3700v4 | \
wndr4300)
	ucidef_set_led_netdev "wan" "WAN (green)" "netgear:green:wan" "eth0.2"
	ucidef_set_led_usbdev "usb" "USB" "netgear:green:usb" "1-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "netgear:green:wlan2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "netgear:blue:wlan5g" "phy1tpt"
	;;

whr-g301n |\
whr-hp-g300n |\
whr-hp-gn)
	ucidef_set_led_netdev "wan" "WAN" "buffalo:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "buffalo:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "buffalo:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "buffalo:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "buffalo:green:lan4" "switch0" "0x10"
	;;

wlae-ag300n)
	ucidef_set_led_netdev "wireless" "WIRELESS" "buffalo:green:wireless" "wlan0"
	;;

wnr2000-v4)
	ucidef_set_led_netdev "wan" "WAN" "netgear:green:wan" "eth0"
	ucidef_set_led_netdev "wlan" "WLAN" "netgear:blue:wlan" "wlan0"
	ucidef_set_led_switch "lan1" "LAN1" "netgear:amber:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "netgear:amber:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "netgear:amber:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "netgear:amber:lan4" "switch0" "0x10"
	ucidef_set_led_usbdev "usb" "USB" "netgear:amber:status" "1-1"
    ;;

wzr-hp-ag300h)
	ucidef_set_led_default "diag" "DIAG" "buffalo:red:diag" "0"
	ucidef_set_led_netdev "router" "ROUTER" "buffalo:green:router" "eth1"
	ucidef_set_led_usbdev "usb" "USB" "buffalo:green:usb" "1-1"
	;;

wzr-hp-g300nh)
	ucidef_set_led_wlan "wlan" "Wireless" "buffalo:green:wireless" "phy0tpt"
	ucidef_set_led_netdev "router" "Router" "buffalo:green:router" "eth1"
	ucidef_set_led_usbdev "usb" "USB" "buffalo:blue:usb" "1-1"
	;;

zcn-1523h-2)
	ucidef_set_led_netdev "lan1" "lan1" "zcn-1523h:green:lan1" "eth0"
	;;

zcn-1523h-5)
	ucidef_set_led_netdev "lan1" "lan1" "zcn-1523h:green:lan1" "eth0"
	ucidef_set_led_netdev "lan2" "lan2" "zcn-1523h:green:lan2" "eth1"
	;;
esac

ucidef_commit_leds

exit 0
