From: Pontus Fuchs <pontusf@broadcom.com>
Date: Thu, 11 Jun 2015 00:12:17 +0200
Subject: [PATCH] brcmfmac: Check if firmware supports p2p

Add a feature flag to reflect the firmware's p2p capability.

Reviewed-by: Pieter-Paul Giesberts <pieterpg@broadcom.com>
Reviewed-by: Hante Meuleman <meuleman@broadcom.com>
Reviewed-by: Arend Van Spriel <arend@broadcom.com>
Signed-off-by: Pontus Fuchs <pontusf@broadcom.com>
Signed-off-by: Arend van Spriel <arend@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---

--- a/drivers/net/wireless/brcm80211/brcmfmac/feature.c
+++ b/drivers/net/wireless/brcm80211/brcmfmac/feature.c
@@ -129,6 +129,7 @@ void brcmf_feat_attach(struct brcmf_pub
 		brcmf_feat_iovar_int_get(ifp, BRCMF_FEAT_WOWL, "wowl");
 	if (drvr->bus_if->chip != BRCM_CC_43362_CHIP_ID)
 		brcmf_feat_iovar_int_set(ifp, BRCMF_FEAT_MBSS, "mbss", 0);
+	brcmf_feat_iovar_int_get(ifp, BRCMF_FEAT_P2P, "p2p");
 
 	/* set chip related quirks */
 	switch (drvr->bus_if->chip) {
--- a/drivers/net/wireless/brcm80211/brcmfmac/feature.h
+++ b/drivers/net/wireless/brcm80211/brcmfmac/feature.h
@@ -23,12 +23,14 @@
  * MCHAN: multi-channel for concurrent P2P.
  * PNO: preferred network offload.
  * WOWL: Wake-On-WLAN.
+ * P2P: peer-to-peer
  */
 #define BRCMF_FEAT_LIST \
 	BRCMF_FEAT_DEF(MBSS) \
 	BRCMF_FEAT_DEF(MCHAN) \
 	BRCMF_FEAT_DEF(PNO) \
-	BRCMF_FEAT_DEF(WOWL)
+	BRCMF_FEAT_DEF(WOWL) \
+	BRCMF_FEAT_DEF(P2P)
 /*
  * Quirks:
  *
