From: Arend van Spriel <arend@broadcom.com>
Date: Tue, 14 Apr 2015 20:10:31 +0200
Subject: [PATCH] brcmfmac: add support for BCM4358 PCIe device

This patch adds support for the BCM4358 2x2 11ac device.

Reviewed-by: Pieter-Paul Giesberts <pieterpg@broadcom.com>
Signed-off-by: Arend van Spriel <arend@broadcom.com>
---

--- a/drivers/net/wireless/brcm80211/brcmfmac/chip.c
+++ b/drivers/net/wireless/brcm80211/brcmfmac/chip.c
@@ -649,6 +649,7 @@ static u32 brcmf_chip_tcm_rambase(struct
 	case BRCM_CC_43567_CHIP_ID:
 	case BRCM_CC_43569_CHIP_ID:
 	case BRCM_CC_43570_CHIP_ID:
+	case BRCM_CC_4358_CHIP_ID:
 	case BRCM_CC_43602_CHIP_ID:
 		return 0x180000;
 	default:
--- a/drivers/net/wireless/brcm80211/brcmfmac/pcie.c
+++ b/drivers/net/wireless/brcm80211/brcmfmac/pcie.c
@@ -51,6 +51,8 @@ enum brcmf_pcie_state {
 #define BRCMF_PCIE_4356_NVRAM_NAME		"brcm/brcmfmac4356-pcie.txt"
 #define BRCMF_PCIE_43570_FW_NAME		"brcm/brcmfmac43570-pcie.bin"
 #define BRCMF_PCIE_43570_NVRAM_NAME		"brcm/brcmfmac43570-pcie.txt"
+#define BRCMF_PCIE_4358_FW_NAME			"brcm/brcmfmac4358-pcie.bin"
+#define BRCMF_PCIE_4358_NVRAM_NAME		"brcm/brcmfmac4358-pcie.txt"
 
 #define BRCMF_PCIE_FW_UP_TIMEOUT		2000 /* msec */
 
@@ -189,6 +191,8 @@ MODULE_FIRMWARE(BRCMF_PCIE_4356_FW_NAME)
 MODULE_FIRMWARE(BRCMF_PCIE_4356_NVRAM_NAME);
 MODULE_FIRMWARE(BRCMF_PCIE_43570_FW_NAME);
 MODULE_FIRMWARE(BRCMF_PCIE_43570_NVRAM_NAME);
+MODULE_FIRMWARE(BRCMF_PCIE_4358_FW_NAME);
+MODULE_FIRMWARE(BRCMF_PCIE_4358_NVRAM_NAME);
 
 
 struct brcmf_pcie_console {
@@ -1333,6 +1337,10 @@ static int brcmf_pcie_get_fwnames(struct
 		fw_name = BRCMF_PCIE_43570_FW_NAME;
 		nvram_name = BRCMF_PCIE_43570_NVRAM_NAME;
 		break;
+	case BRCM_CC_4358_CHIP_ID:
+		fw_name = BRCMF_PCIE_4358_FW_NAME;
+		nvram_name = BRCMF_PCIE_4358_NVRAM_NAME;
+		break;
 	default:
 		brcmf_err("Unsupported chip 0x%04x\n", devinfo->ci->chip);
 		return -ENODEV;
@@ -1850,6 +1858,7 @@ static struct pci_device_id brcmf_pcie_d
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_4356_DEVICE_ID),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43567_DEVICE_ID),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43570_DEVICE_ID),
+	BRCMF_PCIE_DEVICE(BRCM_PCIE_4358_DEVICE_ID),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43602_DEVICE_ID),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43602_2G_DEVICE_ID),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43602_5G_DEVICE_ID),
--- a/drivers/net/wireless/brcm80211/include/brcm_hw_ids.h
+++ b/drivers/net/wireless/brcm80211/include/brcm_hw_ids.h
@@ -45,6 +45,7 @@
 #define BRCM_CC_43567_CHIP_ID		43567
 #define BRCM_CC_43569_CHIP_ID		43569
 #define BRCM_CC_43570_CHIP_ID		43570
+#define BRCM_CC_4358_CHIP_ID		0x4358
 #define BRCM_CC_43602_CHIP_ID		43602
 
 /* USB Device IDs */
@@ -59,6 +60,7 @@
 #define BRCM_PCIE_4356_DEVICE_ID	0x43ec
 #define BRCM_PCIE_43567_DEVICE_ID	0x43d3
 #define BRCM_PCIE_43570_DEVICE_ID	0x43d9
+#define BRCM_PCIE_4358_DEVICE_ID	0x43e9
 #define BRCM_PCIE_43602_DEVICE_ID	0x43ba
 #define BRCM_PCIE_43602_2G_DEVICE_ID	0x43bb
 #define BRCM_PCIE_43602_5G_DEVICE_ID	0x43bc
