--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -196,6 +196,17 @@ config ATH79_MACH_F9K1115V2
 	select ATH79_DEV_USB
 	select ATH79_DEV_WMAC
 
+config ATH79_MACH_EPG5000
+	bool "EnGenius EPG5000 board support"
+	select SOC_QCA955X
+	select ATH79_DEV_ETH
+	select ATH79_DEV_GPIO_BUTTONS
+	select ATH79_DEV_LEDS_GPIO
+	select ATH79_DEV_M25P80
+	select ATH79_DEV_USB
+	select ATH79_DEV_WMAC
+	select ATH79_NVRAM
+
 config ATH79_MACH_ESR1750
 	bool "EnGenius ESR1750 board support"
 	select SOC_QCA955X
--- a/arch/mips/ath79/Makefile
+++ b/arch/mips/ath79/Makefile
@@ -71,6 +71,7 @@ obj-$(CONFIG_ATH79_MACH_EAP300V2)	+= mac
 obj-$(CONFIG_ATH79_MACH_EAP7660D)	+= mach-eap7660d.o
 obj-$(CONFIG_ATH79_MACH_EL_M150)	+= mach-el-m150.o
 obj-$(CONFIG_ATH79_MACH_EL_MINI)	+= mach-el-mini.o
+obj-$(CONFIG_ATH79_MACH_EPG5000)	+= mach-epg5000.o
 obj-$(CONFIG_ATH79_MACH_ESR1750)	+= mach-esr1750.o
 obj-$(CONFIG_ATH79_MACH_F9K1115V2)	+= mach-f9k1115v2.o
 obj-$(CONFIG_ATH79_MACH_GL_INET)	+= mach-gl-inet.o
--- a/arch/mips/ath79/machtypes.h
+++ b/arch/mips/ath79/machtypes.h
@@ -61,6 +61,7 @@ enum ath79_mach_type {
 	ATH79_MACH_EL_M150,		/* EasyLink EL-M150 */
 	ATH79_MACH_EL_MINI,		/* EasyLink EL-MINI */
 	ATH79_MACH_ESR1750,		/* EnGenius ESR1750 */
+	ATH79_MACH_EPG5000,		/* EnGenius EPG5000 */
 	ATH79_MACH_F9K1115V2,		/* Belkin AC1750DB */
 	ATH79_MACH_GL_INET,		/* GL-CONNECT GL-INET */
 	ATH79_MACH_GS_OOLITE,           /* GS OOLITE V1.0 */
