From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Mon, 8 Jun 2015 16:59:31 +0200
Subject: [PATCH] brcmfmac: use bcm47xx platform NVRAM as fallback
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---

--- a/drivers/net/wireless/brcm80211/brcmfmac/firmware.c
+++ b/drivers/net/wireless/brcm80211/brcmfmac/firmware.c
@@ -19,6 +19,9 @@
 #include <linux/device.h>
 #include <linux/firmware.h>
 #include <linux/module.h>
+#if IS_ENABLED(CONFIG_BCM47XX_NVRAM)
+#include <linux/bcm47xx_nvram.h>
+#endif
 
 #include "debug.h"
 #include "firmware.h"
@@ -424,17 +427,42 @@ struct brcmf_fw {
 static void brcmf_fw_request_nvram_done(const struct firmware *fw, void *ctx)
 {
 	struct brcmf_fw *fwctx = ctx;
+#if IS_ENABLED(CONFIG_BCM47XX_NVRAM)
+	const u8 *bcm47xx_nvram = NULL;
+	size_t bcm47xx_nvram_len;
+#endif
+	const u8 *data = NULL;
+	size_t data_len;
 	u32 nvram_length = 0;
 	void *nvram = NULL;
 
 	brcmf_dbg(TRACE, "enter: dev=%s\n", dev_name(fwctx->dev));
-	if (!fw && !(fwctx->flags & BRCMF_FW_REQ_NV_OPTIONAL))
+	if (fw) {
+		data = fw->data;
+		data_len = fw->size;
+	}
+#if IS_ENABLED(CONFIG_BCM47XX_NVRAM)
+	else {
+		bcm47xx_nvram = bcm47xx_nvram_get_contents(&bcm47xx_nvram_len);
+		if (bcm47xx_nvram) {
+			data = bcm47xx_nvram;
+			data_len = bcm47xx_nvram_len;
+			brcmf_err("Found platform NVRAM (%zu B)\n", data_len);
+		}
+	}
+#endif
+	if (!data && !(fwctx->flags & BRCMF_FW_REQ_NV_OPTIONAL))
 		goto fail;
 
-	if (fw) {
-		nvram = brcmf_fw_nvram_strip(fw->data, fw->size, &nvram_length,
+	if (data) {
+		nvram = brcmf_fw_nvram_strip(data, data_len, &nvram_length,
 					     fwctx->domain_nr, fwctx->bus_nr);
-		release_firmware(fw);
+		if (fw)
+			release_firmware(fw);
+#if IS_ENABLED(CONFIG_BCM47XX_NVRAM)
+		if (bcm47xx_nvram)
+			bcm47xx_nvram_release_contents(bcm47xx_nvram);
+#endif
 		if (!nvram && !(fwctx->flags & BRCMF_FW_REQ_NV_OPTIONAL))
 			goto fail;
 	}
--- a/drivers/net/wireless/brcm80211/brcmfmac/debug.h
+++ b/drivers/net/wireless/brcm80211/brcmfmac/debug.h
@@ -17,6 +17,8 @@
 #ifndef BRCMFMAC_DEBUG_H
 #define BRCMFMAC_DEBUG_H
 
+#include <linux/net.h>
+
 /* message levels */
 #define BRCMF_TRACE_VAL		0x00000002
 #define BRCMF_INFO_VAL		0x00000004
