--- a/drivers/leds/trigger/Kconfig
+++ b/drivers/leds/trigger/Kconfig
@@ -108,4 +108,8 @@ config LEDS_TRIGGER_CAMERA
 	  This enables direct flash/torch on/off by the driver, kernel space.
 	  If unsure, say Y.
 
+config LEDS_TRIGGER_MORSE
+	tristate "LED Morse Trigger"
+	depends on LEDS_TRIGGERS
+
 endif # LEDS_TRIGGERS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -62,3 +62,4 @@ obj-$(CONFIG_LEDS_DAC124S085)		+= leds-d
 
 # LED Triggers
 obj-$(CONFIG_LEDS_TRIGGERS)		+= trigger/
+obj-$(CONFIG_LEDS_TRIGGER_MORSE)	+= ledtrig-morse.o
--- a/drivers/leds/ledtrig-morse.c
+++ b/drivers/leds/ledtrig-morse.c
@@ -26,7 +26,6 @@
 #include <linux/list.h>
 #include <linux/spinlock.h>
 #include <linux/device.h>
-#include <linux/sysdev.h>
 #include <linux/timer.h>
 #include <linux/ctype.h>
 #include <linux/leds.h>
