From 74b7eaf75fc6eb86292056ef705e543f9cd6086b Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Sun, 18 Aug 2013 09:57:58 +0200
Subject: [PATCH] rt2x00: rt2800lib: use correct beacon count for RT3883

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/rt2x00/rt2800lib.c |    3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/rt2x00/rt2800lib.c
@@ -8428,7 +8428,8 @@ int rt2800_probe_hw(struct rt2x00_dev *r
 	if (rt2x00_rt(rt2x00dev, RT3593))
 		__set_bit(RT2800_HAS_HIGH_SHARED_MEM, &drv_data->rt2800_flags);
 
-	if (rt2x00_rt(rt2x00dev, RT3593))
+	if (rt2x00_rt(rt2x00dev, RT3593) ||
+	    rt2x00_rt(rt2x00dev, RT3883))
 		drv_data->hw_beacon_count = 16;
 	else
 		drv_data->hw_beacon_count = 8;
