From: Hante Meuleman <meuleman@broadcom.com>
Date: Wed, 18 Mar 2015 13:25:24 +0100
Subject: [PATCH] brcmfmac: Remove unnecessary new-line in pcie console
 logging.

Reviewed-by: Arend Van Spriel <arend@broadcom.com>
Reviewed-by: Pieter-Paul Giesberts <pieterpg@broadcom.com>
Signed-off-by: Hante Meuleman <meuleman@broadcom.com>
Signed-off-by: Arend van Spriel <arend@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---

--- a/drivers/net/wireless/brcm80211/brcmfmac/pcie.c
+++ b/drivers/net/wireless/brcm80211/brcmfmac/pcie.c
@@ -651,10 +651,9 @@ static void brcmf_pcie_bus_console_read(
 			console->log_str[console->log_idx] = ch;
 			console->log_idx++;
 		}
-
 		if (ch == '\n') {
 			console->log_str[console->log_idx] = 0;
-			brcmf_dbg(PCIE, "CONSOLE: %s\n", console->log_str);
+			brcmf_dbg(PCIE, "CONSOLE: %s", console->log_str);
 			console->log_idx = 0;
 		}
 	}
