/dts-v1/;

/include/ "danube.dtsi"

/ {
	model = "BTHOMEHUBV2B - BT Home Hub 2B";  /* SoC: Lantiq Danube-S PSB 50712 @ 333MHz V1.3/1.5 */

	chosen {
		bootargs = "console=ttyLTQ0,115200 init=/etc/preinit";
	};

	memory@0 {				  /* RAM: Samsung K4H511638F-LC 64MB */
		reg = <0x0 0x4000000>;
	};

	sram@1F000000 {
		vmmc@107000 {
			status = "okay";
			gpios = <&gpio 31 0>;
		};
	};

	fpi@10000000 {
		#address-cells = <1>;
		#size-cells = <1>;
		localbus@0 {
			#address-cells = <2>;
			#size-cells = <1>;
			ranges = <0 0 0x0 0x3ffffff /* addrsel0 */
				1 0 0x4000000 0x4000010>; /* addsel1 */
			compatible = "lantiq,localbus", "simple-bus";

			nor-boot@0 {				/* NOR Flash: Spansion S29AL004D 512KB */
				compatible = "lantiq,nor";	/* "AMD AM29LV400BB" compatible on 3.3.8 */
				lantiq,cs = <0>;
				bank-width = <2>;
				reg = <0 0x0 0x80000>;
				#address-cells = <1>;
				#size-cells = <1>;

				partition@0 {
					label = "uboot";
					reg = <0x00000 0x40000>; /* 256KB */
				};

				partition@40000 {
					label = "uboot_env";
					reg = <0x40000 0x10000>; /* 64KB */
				};

				partition@50000 {
					label = "rg_conf_1";
					reg = <0x50000 0x10000>;
				};

				partition@60000 {
					label = "rg_conf_2";
					reg = <0x60000 0x10000>;
				};

				partition@70000 {
					label = "rg_conf_factory";
					reg = <0x70000 0x10000>;
				};
			};

			nand-parts@0 {		  /* NAND Flash: Samsung K9F5608U0D-JIB0 32MB */
				compatible = "gen_nand", "lantiq,nand-xway";
				lantiq,cs = <1>;
				bank-width = <2>;
				reg = <1 0x0 0x2000000 >;
				#address-cells = <1>;
				#size-cells = <1>;
				req-mask = <0x1>;  /* PCI request lines to mask during NAND access */

				ath9k_cal: partition@0 {
					label = "art";	   /* Atheros 9160 wifi b/g/n radio EEPROM */
					reg = <0x00000 0x4000>;
					read-only;
				};

				partition@4000 {
					label = "kernel";
					reg = <0x4000 0x200000>;
				};

				partition@164000 {
					label = "ubi";
					reg = <0x204000 0x1DFC000>;
				};

			};


			ath9k_eep {
				compatible = "ath9k,eeprom";
				ath,eep-flash = <&ath9k_cal 0x0000>;
				ath,mac-increment = <1>;
				ath,pci-slot = <14>;
				ath,eep-endian;
			};
		};

		gpio: pinmux@E100B10 {
			compatible = "lantiq,pinctrl-xway";
			pinctrl-names = "default";
			pinctrl-0 = <&state_default>;

			#gpio-cells = <2>;
			gpio-controller;
			reg = <0xE100B10 0xA0>;

			state_default: pinmux {
				stp {
					lantiq,groups = "stp";
					lantiq,function = "stp";
					lantiq,output = <1>;
					lantiq,open-drain = <0>;
					lantiq,pull = <0>;
				};
				nand_out {
					lantiq,groups = "nand cle", "nand ale";
					lantiq,function = "ebu";
					lantiq,output = <1>;
					lantiq,open-drain = <0>;
					lantiq,pull = <0>;
				};
				nand_cs1 {
					lantiq,groups = "nand cs1";
					lantiq,function = "ebu";
					lantiq,open-drain = <0>;
					lantiq,pull = <0>;
				};
				exin {
					lantiq,groups = "exin1";
					lantiq,function = "exin";
				};
				pci_in {
					lantiq,groups = "req1";
					lantiq,function = "pci";
					lantiq,output = <0>;
					lantiq,open-drain = <1>;
					lantiq,pull = <2>;
				};
				pci_out {
					lantiq,groups = "gnt1";
					lantiq,function = "pci";
					lantiq,output = <1>;
					lantiq,open-drain = <0>;
					lantiq,pull = <0>;
				};

				pci_rst {
					lantiq,pins = "io21";
					lantiq,output = <1>;
					lantiq,open-drain = <0>;
				};

				btn_in {
					lantiq,pins = "io2", "io15", "io22";
					lantiq,output = <0>;
					lantiq,open-drain = <1>;
					lantiq,pull = <2>;
				};
			};
		};

		etop@E180000 {
			compatible = "lantiq,etop-xway";
			reg = <0xE180000 0x40000>;
			interrupt-parent = <&icu0>;
			interrupts = <73 78>;
			phy-mode = "rmii";
			mac-address = [ 00 11 22 33 44 55 ];
		};

		ifxhcd@E101000 {
			status = "okay";
		};

		stp0: stp@E100BB0 {
			status = "okay";
			#gpio-cells = <2>;
			compatible = "lantiq,gpio-stp-xway";
			gpio-controller;
			reg = <0xE100BB0 0x40>;

			lantiq,shadow = <0xfff>;
			lantiq,groups = <0x3>;
		};

		pci@E105400 {
			status = "okay";
			lantiq,bus-clock = <33333333>;
			interrupt-map-mask = <0xf800 0x0 0x0 0x7>;
			interrupt-map = <0x7000 0 0 1 &icu0 30 1>;
			gpio-reset = <&gpio 21 0>;
			req-mask = <0x1>;		 /* GNT1 */
		};

	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 2 1>;
			linux,code = <0x198>;
		};
		findhandset {
			label = "findhandset";
			gpios = <&gpio 15 1>;
			linux,code = <0x101>;
		};
		wps {
			label = "wps";
			gpios = <&gpio 22 1>;
			linux,code = <0x211>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		upgrading-orange {
			label = "soc:orange:upgrading";
			gpios = <&stp0 5 0>;
		};

		phone-orange {
			label = "soc:orange:phone";
			gpios = <&stp0 6 0>;
		};
		phone-blue {
			label = "soc:blue:phone";
			gpios = <&stp0 7 0>;
		};

		wireless-orange {
			label = "soc:orange:wireless";
			gpios = <&stp0 8 0>;
		};
		wireless-blue {
			label = "soc:blue:wireless";
			gpios = <&stp0 9 0>;
		};

		broadband-red {
			label = "soc:red:broadband";
			gpios = <&stp0 10 0>;
		};
		broadband-orange {
			label = "soc:orange:broadband";
			gpios = <&stp0 11 0>;
		};
		broadband-blue {
			label = "soc:blue:broadband";
			gpios = <&stp0 12 0>;
		};

		power-red {
			label = "soc:red:power";
			gpios = <&stp0 13 0>;
		};
		power-orange {
			label = "soc:orange:power";
			gpios = <&stp0 14 0>;
		};
		power-blue {
			label = "soc:blue:power";
			gpios = <&stp0 15 0>;
		};
	};

};

