From 2a725b6c8a9f4454363a73acb34c6cfff9390911 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Tue, 3 Feb 2015 11:41:38 +0000
Subject: [PATCH 101/114] BCM270x_DT: Add i2c0_baudrate and i2c1_baudrate
 parameters

---
 arch/arm/boot/dts/bcm2708-rpi-b-plus.dts | 2 ++
 arch/arm/boot/dts/bcm2708-rpi-b.dts      | 2 ++
 arch/arm/boot/dts/bcm2709-rpi-2-b.dts    | 2 ++
 3 files changed, 6 insertions(+)

--- a/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
@@ -93,6 +93,8 @@
 		spi = <&spi0>,"status";
 		i2c0 = <&i2c0>,"status";
 		i2c1 = <&i2c1>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
 
 		act_led_gpio = <&act_led>,"gpios:4";
 		act_led_activelow = <&act_led>,"gpios:8";
--- a/arch/arm/boot/dts/bcm2708-rpi-b.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-b.dts
@@ -93,6 +93,8 @@
 		spi = <&spi0>,"status";
 		i2c0 = <&i2c0>,"status";
 		i2c1 = <&i2c1>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
 
 		act_led_gpio = <&act_led>,"gpios:4";
 		act_led_activelow = <&act_led>,"gpios:8";
--- a/arch/arm/boot/dts/bcm2709-rpi-2-b.dts
+++ b/arch/arm/boot/dts/bcm2709-rpi-2-b.dts
@@ -93,6 +93,8 @@
 		spi = <&spi0>,"status";
 		i2c0 = <&i2c0>,"status";
 		i2c1 = <&i2c1>,"status";
+		i2c0_baudrate = <&i2c0>,"clock-frequency:0";
+		i2c1_baudrate = <&i2c1>,"clock-frequency:0";
 
 		act_led_gpio = <&act_led>,"gpios:4";
 		act_led_activelow = <&act_led>,"gpios:8";
