From: Vineet Gupta <Vineet.Gupta1@synopsys.com>
Date: Thu, 9 Jul 2015 13:43:18 +0530
Subject: [PATCH] brcmfmac: dhd_sdio.c: use existing atomic_or primitive

There's already a generic implementation so use that instead.

Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---

--- a/drivers/net/wireless/brcm80211/brcmfmac/sdio.c
+++ b/drivers/net/wireless/brcm80211/brcmfmac/sdio.c
@@ -2564,15 +2564,6 @@ static inline void brcmf_sdio_clrintr(st
 	}
 }
 
-static void atomic_orr(int val, atomic_t *v)
-{
-	int old_val;
-
-	old_val = atomic_read(v);
-	while (atomic_cmpxchg(v, old_val, val | old_val) != old_val)
-		old_val = atomic_read(v);
-}
-
 static int brcmf_sdio_intr_rstatus(struct brcmf_sdio *bus)
 {
 	struct brcmf_core *buscore;
@@ -2595,7 +2586,7 @@ static int brcmf_sdio_intr_rstatus(struc
 	if (val) {
 		brcmf_sdiod_regwl(bus->sdiodev, addr, val, &ret);
 		bus->sdcnt.f1regdata++;
-		atomic_orr(val, &bus->intstatus);
+		atomic_or(val, &bus->intstatus);
 	}
 
 	return ret;
@@ -2712,7 +2703,7 @@ static void brcmf_sdio_dpc(struct brcmf_
 
 	/* Keep still-pending events for next scheduling */
 	if (intstatus)
-		atomic_orr(intstatus, &bus->intstatus);
+		atomic_or(intstatus, &bus->intstatus);
 
 	brcmf_sdio_clrintr(bus);
 
