From f1ee1275f65e87e035260f4d09a0f0ba98c6854d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Sun, 21 Jun 2015 12:56:32 +0200
Subject: [PATCH] ARM: BCM5301X: Set vcc-gpio for USB controllers
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts | 20 ++++++++++++++++++++
 arch/arm/boot/dts/bcm4708-netgear-r6250.dts       | 11 +++++++++++
 2 files changed, 31 insertions(+)

--- a/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts
+++ b/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts
@@ -25,6 +25,26 @@
 		       0x88000000 0x18000000>;
 	};
 
+	axi@18000000 {
+		usb2@21000 {
+			reg = <0x00021000 0x1000>;
+
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			vcc-gpio = <&chipcommon 9 GPIO_ACTIVE_HIGH>;
+		};
+
+		usb3@23000 {
+			reg = <0x00023000 0x1000>;
+
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			vcc-gpio = <&chipcommon 10 GPIO_ACTIVE_LOW>;
+		};
+	};
+
 	spi {
 		compatible = "spi-gpio";
 		num-chipselects = <1>;
--- a/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
@@ -35,6 +35,17 @@
 		};
 	};
 
+	axi@18000000 {
+		usb3@23000 {
+			reg = <0x00023000 0x1000>;
+
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			vcc-gpio = <&chipcommon 0 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
