From 0253d14782f80cfd1741d4ddd82b83dd7d44a91e Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Mon, 28 Jul 2014 22:44:59 +0200
Subject: [PATCH] ARM: dts: sun7i: Add spi0_pins_a pinctrl setting

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 7 +++++++
 1 file changed, 7 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -784,6 +784,13 @@
 				allwinner,pull = <0>;
 			};
 
+			spi0_pins_a: spi0@0 {
+				allwinner,pins = "PI10", "PI11", "PI12", "PI13", "PI14";
+				allwinner,function = "spi0";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
 			spi1_pins_a: spi1@0 {
 				allwinner,pins = "PI16", "PI17", "PI18", "PI19";
 				allwinner,function = "spi1";
