A platform_driver does not need to set an owner, it will be populated by the
driver core.

Signed-off-by: Wolfram Sang <wsa@the-dreams.de>

--- a/drivers/gpio/gpio-mvebu.c
+++ b/drivers/gpio/gpio-mvebu.c
@@ -836,7 +836,6 @@ static int mvebu_gpio_probe(struct platf
 static struct platform_driver mvebu_gpio_driver = {
 	.driver		= {
 		.name	        = "mvebu-gpio",
-		.owner	        = THIS_MODULE,
 		.of_match_table = mvebu_gpio_of_match,
 	},
 	.probe		= mvebu_gpio_probe,
