Subject: [PATCH] ARM: BCM5301X: Add profiling support

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
---
--- a/arch/arm/boot/dts/bcm5301x.dtsi
+++ b/arch/arm/boot/dts/bcm5301x.dtsi
@@ -82,6 +82,13 @@
 		};
 	};
 
+	pmu {
+		compatible = "arm,cortex-a9-pmu";
+		interrupts =
+			<GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>,
+			<GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
+	};
+
 	clocks {
 		#address-cells = <1>;
 		#size-cells = <0>;
