From: Hante Meuleman <meuleman@broadcom.com>
Date: Tue, 14 Apr 2015 20:10:32 +0200
Subject: [PATCH] brcmfmac: add additional 43602 pcie device id.

Reviewed-by: Arend Van Spriel <arend@broadcom.com>
Reviewed-by: Pieter-Paul Giesberts <pieterpg@broadcom.com>
Signed-off-by: Hante Meuleman <meuleman@broadcom.com>
Signed-off-by: Arend van Spriel <arend@broadcom.com>
---

--- a/drivers/net/wireless/brcm80211/brcmfmac/pcie.c
+++ b/drivers/net/wireless/brcm80211/brcmfmac/pcie.c
@@ -1862,6 +1862,7 @@ static struct pci_device_id brcmf_pcie_d
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43602_DEVICE_ID),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43602_2G_DEVICE_ID),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43602_5G_DEVICE_ID),
+	BRCMF_PCIE_DEVICE(BRCM_PCIE_43602_RAW_DEVICE_ID),
 	{ /* end: all zeroes */ }
 };
 
--- a/drivers/net/wireless/brcm80211/include/brcm_hw_ids.h
+++ b/drivers/net/wireless/brcm80211/include/brcm_hw_ids.h
@@ -64,6 +64,7 @@
 #define BRCM_PCIE_43602_DEVICE_ID	0x43ba
 #define BRCM_PCIE_43602_2G_DEVICE_ID	0x43bb
 #define BRCM_PCIE_43602_5G_DEVICE_ID	0x43bc
+#define BRCM_PCIE_43602_RAW_DEVICE_ID	43602
 
 /* brcmsmac IDs */
 #define BCM4313_D11N2G_ID	0x4727	/* 4313 802.11n 2.4G device */
